>> MIB - Management Information Base
>> Table: ospfErr - (.1.3.6.1.4.1.272.4.5.11)
ospfErr
OID | Name | Type | Access
.1 | OspfBadVersion | Counter | R
.2 | OspfBadPacketType | Counter | R
.3 | OspfBadChecksum | Counter | R
.4 | IpBadDestination | Counter | R
.5 | OspfBadAreaId | Counter | R
.6 | OspfAuthenticationFailed | Counter | R
.7 | OspfUnknownNeighbor | Counter | R
.8 | HelloNetmaskMismatch | Counter | R
.9 | HelloDeadTimerMismatch | Counter | R
.10 | HelloTimerMismatch | Counter | R
.11 | HelloOptionMismatch | Counter | R
.12 | OspfRouterIdConfusion | Counter | R
.13 | OspfUnknownLsaType | Counter | R
.14 | DdOptionMismatch | Counter | R
.15 | DdNeighborStateLow | Counter | R
.16 | LsackBadAck | Counter | R
.17 | LsackDuplicateAck | Counter | R
.18 | LsreqBadRequest | Counter | R
.19 | LsreqNeighborStateLow | Counter | R
.20 | LsupdNeighborStateLow | Counter | R
.21 | LsupdBadLsaChecksum | Counter | R
.22 | LsupdNewerSelfgenLsa | Counter | R
.23 | LsupdLessRecentLsa | Counter | R
OspfBadVersion
Counts the number of OSPF packets received with bad version number.
OspfBadPacketType
Counts the number of OSPF packets received with bad packet type.
OspfBadChecksum
Counts the number of OSPF packets received with bad checksum.
IpBadDestination
Counts the number of OSPF packets received with bad destination IP address.
OspfBadAreaId
Counts the number of OSPF packets with the wrong area field.
OspfAuthenticationFailed
Counts the number of OSPF packets with wrong authentication.
OspfUnknownNeighbor
Counts the number of OSPF packets received from an unknown neighbor.
HelloNetmaskMismatch
Counts the number of Hello packets received with wrong network mask.
HelloDeadTimerMismatch
Counts the number of OSPF Hello packets where the DeadTimer was not equal to the DeadTimer of the associated interface.
HelloTimerMismatch
Counts the number of OSPF Hello packets where the HelloTimer was not equal to the DeadTimer of the associated interface.
HelloOptionMismatch
Counts the number of OSPF Hello packets with bad options.
OspfRouterIdConfusion
Counts the number of packets received that used our own router id.
OspfUnknownLsaType
Counts the number of unknown LSAs received.
DdOptionMismatch
Counts the number of OSPF DD packets with bad options.
DdNeighborStateLow
Counts the number of OSPF DD packets received then the neighbor was in the wrong state.
LsackBadAck
Counts the number of OSPF LS Acknowledge packets received that were not exactly found on the retransmission list of that neighbor, i.e. with the wrong sequence number or checksum.
LsackDuplicateAck
Counts the number of OSPF LS Acknowledge packets received that were not found on the retransmission list of that neighbor.
LsreqBadRequest
Counts the number of requests for LSAs that were not found in the database.
LsreqNeighborStateLow
Counts the number of OSPF LS Request packets received then the neighbor was in the wrong state.
LsupdNeighborStateLow
Counts the number of OSPF LS Update packets received then the neighbor was in the wrong state.
LsupdBadLsaChecksum
Counts the number of OSPF LS Update packets with bad checksum.
LsupdNewerSelfgenLsa
The router received an instance of one of its self-originated advertisements that is considered to be more recent.
LsupdLessRecentLsa
The router received an instance of an advertisement that is considered to be less recent than the database copy.

MIB Reference to Software Version 9.1.2 generated on 2012/09/25. Provided by webmaster@teldat.de Copyright ©2012 by Teldat GmbH