>> MIB - Management Information Base
>> Table: systemPhoneFwuProcessTable - (.1.3.6.1.4.1.272.4.64.5.3.1)
Description: This table contains information of firmware update of system phones.
systemPhoneFwuProcessTable
OID | Name | Type | Access
.1 | Index | SystelTerminalIndex | RW
.2 | StartNow | ENUM | RW
.3 | StartSchedule | ENUM | RW
.4 | Status | ENUM | R
.5 | Result | ENUM | R
.6 | Progress | INTEGER | R
.7 | UnknownMsgCounter | Unsigned32 | R
.8 | TimeoutCounter | Unsigned32 | R
.9 | AdminStatus | ENUM | D
Index
A reference to the systemPhoneTable (or mpsTerminalTable). Range: 1 to 65535
StartNow
This variable contains the user input in a boolean value to immediately update the firmware of this device. Enumerations: true (1) false (2)
StartSchedule
If this variable is true, the firmwareupdate starts scheduled. The periode of firmware updates is defined in systemPhoneFwuServerTable. Enumerations: true (1) false (2)
Status
Status of system phone firmware update: done -> there is no firmware update in time running -> firmwareupdate is actually running waiting -> because lack of system ressources the scheduled or immediately started firmware update is in waiting mode. Enumerations: done (1) running (2) waiting (3)
Result
Result of system phone firmware update: idle -> initial value ok -> firmware update is successfully completed failed -> an error occurred during the firmware update process. Enumerations: idle (1) ok (2) failed (3)
Progress
Progress of system phone firmware update. Range: 0 to 100
UnknownMsgCounter
Statistic value which shows the received unknown messages of internal firmware download server during the firmware update.
TimeoutCounter
Statistic value which shows the occured timeouts during the firmware update.
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)

MIB Reference to Software Version 9.1.2 generated on 2012/09/25. Provided by webmaster@teldat.de Copyright ©2012 by Teldat GmbH