>> MIB - Management Information Base
>> Table: ethPhyTable - (.1.3.6.1.4.1.272.4.45.1.1)
Description: The ethPhyEntry contains configuration and status information of a physical interface associated to one ethernet interface.
ethPhyTable
OID | Name | Type | Access
.1 | PortIndex | INTEGER | R
.2 | ChipVendor | DisplayString | R
.3 | ChipModel | DisplayString | R
.6 | PortLinkStatus | ENUM | R
.7 | PortMdixStatus | ENUM | R
.9 | PortCapabilities | BITS | R
.10 | PortMode | ENUM | RW
.12 | EthAssignedIfIndex | INTEGER | RW
.13 | ExtendedDistance | ENUM | RW
.18 | PortGroup | INTEGER | RW
.21 | PortDescr | DisplayString | RW
.22 | PortFlowControl | ENUM | RW
.23 | PortFlowControlStatus | ENUM | R
PortIndex
The unique ethernet PHY interface index.
ChipVendor
The vendor name or identifier of the PHY or switch detected during hardware scan. Length: 1 to 40
ChipModel
The chip modell/revision of the PHY or switch detected during hardware scan. Length: 1 to 40
PortLinkStatus
This variable indicates link status and autonegotiation results: down(1) -- link down or autonegotiation failed auto-neg-failed(2) -- autonegotiation failed auto-neg-unavail(3) -- autonegotiation not available auto-neg-running(4) -- autonegotiation running auto-full-100(5) -- negotiated 100 mbps/full duplex auto-half-100(6) -- negotiated 100 mbps/half duplex auto-full-10(7) -- negotiated 10 mbps/full duplex auto-half-10(8) -- negotiated 10 mbps/half duplex full-100(9) -- forced mode 100 mbps/full duplex half-100(10) -- forced mode 100 mbps/half duplex full-10(11) -- forced mode 10 mbps/full duplex half-10(12) -- forcde mode 10 mbps/half duplex admin-down(13) -- link set administrative down full-1000(14) -- forced mode 1000 mbps/full duplex Enumerations: down (1) auto-neg-failed (2) auto-neg-unavail (3) auto-neg-running (4) auto-full-100 (5) auto-half-100 (6) auto-full-10 (7) auto-half-10 (8) full-100 (9) half-100 (10) full-10 (11) half-10 (12) admin-down (13) full-1000 (14)
PortMdixStatus
This variable indicates the cables MDIX status if the link is established. Enumerations: normal (1) crossover (2) unknown (3)
PortCapabilities
This bitfield describes what modes the port supports: half-10 : 10Mbit/s half duplex full-10 : 10Mbit/s full duplex half-100 : 100Mbit/s half duplex full-100 : 100Mbit/s full duplex half-1000 : 1000Mbit/s half duplex full-1000 : 1000Mbit/s full duplex autoneg : Autonegotiation supported . Enumerations: half-10 (0) full-10 (1) half-100 (2) full-100 (3) half-1000 (4) full-1000 (5) autoneg (6)
PortMode
The initial mode of the ethernet PHY or switch port: disable(1) -- disconnect from physical line auto(2) -- use default autonegotiation auto-100(3) -- use autonegotiation for 100 mbps only auto-10(4) -- use autonegotiation for 10 mbps only auto-full-100(5) -- auto-negotiate 100 mbps/full-duplex auto-half-100(6) -- auto-negotiate 100 mbps/half-duplex auto-full-10(7) -- auto-negotiate 10 mbps/full-duplex auto-half-10(8) -- auto-negotiate 10 mbps/half-duplex fixed-full-100(9) -- use fixed mode 100 mbps/full-duplex fixed-half-100(10) -- use fixed mode 100 mbps/half-duplex fixed-full-10(11) -- use fixed mode 10 mbps/full-duplex fixed-half-10(12) -- use fixed mode 10 mbps/half-duplex auto-1000(14) -- use autonegotiation for 1000 mbps only fixed-full-1000(15) -- use fixed mode 1000 mbps/full-duplex Enumerations: disable (1) auto (2) auto-100 (3) auto-10 (4) auto-full-100 (5) auto-half-100 (6) auto-full-10 (7) auto-half-10 (8) fixed-full-100 (9) fixed-half-100 (10) fixed-full-10 (11) fixed-half-10 (12) auto-1000 (14) fixed-full-1000 (15)
EthAssignedIfIndex
The Ethernet interface index the PHY or switch port is connected/assigned to. The system will create interfaces as needed, but there can't be more ethernet interfaces than switch ports.
ExtendedDistance
If the PHY supports different receive thresholds depending on the cable length (long-cable > 100 m) and speed (10BaseT) it could be configured by this variable. Enumerations: default (1) short-cable (2) long-cable (3)
PortGroup
The port group this phy is member of. Range: 0 to 99
PortDescr
This object is available to the user for specifying a user-friendly name or tag. Length: 0 to 255
PortFlowControl
If the PHY supports flow control according to IEEE 802.3x flow control can be enabled on that port by setting variable to value 'auto'. This will cause 802.3x to be advertised via that port as well as enabled automatically in case flow control gets negotiated. Value 'disable' keeps flow control from being advertised and, hence, from being used at all. With value 'enable' flow control can be forced to be enabled regardless of any auto-negotiation. Default value is disable. Enumerations: disable (1) enable (2) auto (3)
PortFlowControlStatus
This variable indicates whether flow control according to IEEE 802.3x is currently active on that port. Possible values are ... disabled(1) and enabled(2) Enumerations: disabled (1) enabled (2)

MIB Reference to Software Version 9.1.2 generated on 2012/09/25. Provided by webmaster@teldat.de Copyright ©2012 by Teldat GmbH