>> MIB - Management Information Base
>> Table: capwapBaseParameters - (.1.3.6.1.2.1.60.1.3)
capwapBaseParameters
OID | Name | Type | Access
.1 | MaxRetransmit | Unsigned32 | RW
.2 | ChangeStatePendingTimer | Unsigned32 | RW
.3 | DataCheckTimer | Unsigned32 | RW
.5 | EchoInterval | Unsigned32 | RW
.6 | RetransmitInterval | Unsigned32 | RW
.9 | WaitJoinTimer | Unsigned32 | RW
MaxRetransmit
Represents the maximum number of retransmissions for a given CAPWAP packet before the link layer considers the peer dead. The value of the object is persistent at restart/reboot.
ChangeStatePendingTimer
Represents the maximum time, in seconds, the AC will wait for the Change State Event Request from the WTP after having transmitted a successful Configuration Status Response message. The value is multiplied by the number of WTP's radio-modules. The value of the object is persistent at restart/reboot.
DataCheckTimer
Represents The number of seconds the AC will wait for the Data Channel Keep Alive, which is required by the CAPWAP state machine's Data Check state. The AC resets the state machine if this timer expires prior to transitioning to the next state. The value of the object is persistent at restart/reboot.
EchoInterval
Represents the minimum time, in seconds, between sending Echo Request messages to the AC with which the WTP has joined. The value of the object is persistent at restart/reboot.
RetransmitInterval
Represents the minimum time, in seconds, in which a non-acknowledged CAPWAP packet will be retransmitted. The value of the object is persistent at restart/reboot.
WaitJoinTimer
Represents the maximum time, in seconds, the AC will wait after the DTLS session has been established until it receives the Join Request from the WTP. This timer MUST be greater than 20 seconds. The value of the object is persistent at restart/reboot. Range: 20 to -1

MIB Reference to Software Version 9.1.2 generated on 2012/09/25. Provided by webmaster@teldat.de Copyright ©2012 by Teldat GmbH