>> MIB - Management Information Base
>> Table: wlcWTPGlobalProfileTable - (.1.3.6.1.4.1.272.4.61.1.9.1)
Description: This table cotains WTP debug level settings
wlcWTPGlobalProfileTable
OID | Name | Type | Access
.1 | Index | INTEGER | RW
.3 | DebugType | ENUM | RW
.4 | DebugLevel | ENUM | RW
.5 | AdminStatus | ENUM | D
Index
Unique index of a global profile.
DebugType
Wireless LAN Controler degugging type. With type common(1) debugging messages of authentication, access_point, bridge and client handling will be shown. With type authentication(2) only messages concerning the authentication handling (mainly WPA) will be shown. With type access_point(3) only messages concerning the access_point handling will be shown. With type bridge(4) only messages concerning the bridge handling will be shown. With type client(5) only messages concerning the client (wlanIfType == client) will be shown. With type lowlevel(6) messages concerning the 802.11 layer and lowlevel driver handling will be shown. With type all(7) all messages of all types will be shown. Default is common(1). Additionally within all types messages concerning generally WLAN handling will be shown. Enumerations: common (1) authentication (2) access-point (3) bridge (4) client (5) lowlevel (6) all (7)
DebugLevel
WLC degugging verbosity level. With a higher value more debugging information will be created. Default is normal(2). Enumerations: quiet (1) normal (2) verbose (3) very-verbose (4)
AdminStatus
WLC global AdminStatus. The AP could be used unmanaged(1) and must therefore be configured directly or managed(2) by a WLAN controller. Delete(32) deletes the required profile. Default is managed(1). Enumerations: unmanaged (1) managed (2) delete (32)

MIB Reference to Software Version 9.1.2 generated on 2012/09/25. Provided by webmaster@teldat.de Copyright ©2012 by Teldat GmbH