>> MIB - Management Information Base
>> Table: systemPhoneCapabilityTable - (.1.3.6.1.4.1.272.4.64.3.1.1)
Description: This table contains system phone capabilities which could be partialy specific to phone types (for example the availability of MSN).
systemPhoneCapabilityTable
OID | Name | Type | Access
.1 | DeviceType | ENUM | R
.2 | AvailableMSN | INTEGER | R
.3 | General | BITS | R
.4 | AvailableFunctionKeys | INTEGER | R
DeviceType
Subscripted via the device type of a system phone. Enumerations: cs290 (20) cs410 (22) cs290u (23) cs410u (24) cs400 (25) ips290 (32) ips400 (33) ips290plus (34) s530 (64) s560 (65) ost-40 (144) ost-80 (145)
AvailableMSN
Number of MSNs available in this device.
General
Capabilities of different system phone types: do-not-disturb : (0) DND - Modus not available, (1) DND - Modus available hands-free : (0) Hands free calling not available, cause no mic in system phone integrated, (1) Hands free calling available local-phonebook : (0) Local phonebook not available, (1) Local phonebook available intercom : (0) Intercom not available, (1) Intercom available hotel : (0) Hotel functions (hotelroom keys) not available, (1) Hotel functions available macrokey : (0) Macro key not available (1) Macro key available boss-secretary : (0) Boss-Secretary functions (Boss-,Secretary-,Diversionkey) not available (1) Boss-Secretary functions available key-extension-module : (0) Key-extensions (T400, T400/2, T500) not available (1) Key-extensions available ab-module : (0) Answering machine not available (1) Answering machine available headset-auto-call : (0) Auto-Call-Acceptance (key) available only if headset control (key) is set (1) Auto-Call-Acceptance available (also without headset control (key), via hands-free telephone). extended-status-led : (0) CS/IP system phones don't support the extended status led configuration. (1) NG phones have a bitfield to configure status led on diffenrent events (eg. incoming/missing call or message). conver-disp-settings : (1) Conversation display settings are available (for CS/IP system phones). (0) NG system phones don't support this settings. ng-do-not-disturb : (1) Special Do not disturb settings in GUI for NG system phones is enable. Furthermore, if this bit is set a do not disturb function key is available. (0) Special Do not disturb settings are disabled and no do not disturb function key is available. extended-auto-pick-up : (0) For CS/IP system phones only following values are available for systemPhoneFacAutoCallAcceptTime: immediatly, sec-5, sec-10 (1) For NG system phones further values are available: off, sec-15, sec-20. shift-key : (0) Shift key is not available. (1) Shift key is available. parallel-ringing-key : (0) Parallel ringing key is not available. (1) Parallel ringing key is available. headset-key : (1) Headset key is available. (0) Headset key is not available. NG system phones have their own firmly integrated headset key, so there is no use of this function key. connection-key : (1) Connection key is available. (0) Connection key is not available. NG system phones don't support this kind of key. Enumerations: do-not-disturb (0) hands-free (1) local-phonebook (2) intercom (3) hotel (4) macrokey (5) boss-secretary (6) key-extension-module (7) ab-module (8) headset-auto-call (9) extended-status-led (10) conver-disp-settings (11) ng-do-not-disturb (12) extended-auto-pick-up (13) shift-key (14) parallel-ringing-key (15) headset-key (16) connection-key (17)
AvailableFunctionKeys
Number of (2-level) function keys available on this device.

MIB Reference to Software Version 9.1.2 generated on 2012/09/25. Provided by webmaster@teldat.de Copyright ©2012 by Teldat GmbH