>> MIB - Management Information Base
>> Table: systemPhoneFwuFileTable - (.1.3.6.1.4.1.272.4.64.5.2.1)
Description: This entries only created by the respective device driver.
systemPhoneFwuFileTable
OID | Name | Type | Access
.1 | Index | INTEGER | RW
.2 | Type | ENUM | RW
.3 | Directory | DisplayString | RW
.4 | Name | DisplayString | RW
.5 | Version | DisplayString | RW
.6 | AdminStatus | ENUM | D
Index
A counting index for each firmware file stored on the mounted device. Range: 1 to 65535
Type
Variable contains the phone type of firmware file (stripped out of the header of file). Enumerations: cs290 (20) cs410 (22) cs290u (23) cs410u (24) cs400 (25) ips290 (32) ips400 (33) ips290plus (34) s530 (64) s560 (65) ost-40 (144) ost-80 (145)
Directory
Specifies the complete path/tree where the firmware file can be found on the mounted device. Length: 0 to 255
Name
Simply contains the firmware file name on the mounted device. Length: 0 to 255
Version
Version information of the firmware file stored on sd card (stripped out of the header of file). Version string of elmeg system phones have a size of max. 9 characters. Siemens OpenStage devices have a maximum size of 12. Length: 0 to 20
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)

MIB Reference to Software Version 9.1.2 generated on 2012/09/25. Provided by webmaster@teldat.de Copyright ©2012 by Teldat GmbH