>> MIB - Management Information Base
>> Table: pppPppoeEthDevTable - (.1.3.6.1.4.1.272.4.3.15.1)
Description: .
pppPppoeEthDevTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | RW
.2 | AdminStatus | ENUM | D
.3 | Index | INTEGER | RW
.4 | MaxTxRate | INTEGER | RW
.10 | OperStatus | ENUM | R
.11 | ResidualBlockTime | INTEGER | R
IfIndex
The associated interface index of this entry.
AdminStatus
The administrative this entry. Enumerations: enabled (1) disabled (2) delete (3)
Index
Specifies the first device to be used for PPP over Ethernet (PPPoE) according RFC 2516.
MaxTxRate
Administrative transmit rate limitation needed in order to support scenarios with external XDSL modems. If specified this value will be adopted in associated biboPPPLinkSpeed value. If set to '0' biboPPPLineSpeed is set according the ifSpeed value of the associated Ethernet Device. Range: 0 to 10000000
OperStatus
The PPP-internal operational status of the first device to be used for PPP over Ethernet (PPPoE) according RFC 2516. Enumerations: dormant (1) connecting (2) up (3) blocked (4)
ResidualBlockTime
The remaining time interval till the associated pppPppoeEthDevOperStatus will be changed from blocked(4) to dormant(1) again. Range: 0 to 2147483647

MIB Reference to Software Version 9.1.2 generated on 2012/09/25. Provided by webmaster@teldat.de Copyright ©2012 by Teldat GmbH