>> MIB - Management Information Base
>> Table: systemPhoneFwuServer - (.1.3.6.1.4.1.272.4.64.5.1)
systemPhoneFwuServer
OID | Name | Type | Access
.1 | StartHour | INTEGER | RW
.2 | StartMinute | INTEGER | RW
.3 | EndHour | INTEGER | RW
.4 | EndMinute | INTEGER | RW
.5 | FileStatus | ENUM | RW
.6 | UploadResult | ENUM | R
StartHour
Every day firmware update start time (hour). Range: 0 to 24
StartMinute
Every day firmware update start time (minute). Range: 0 to 60
EndHour
Every day firmware update end time (hour). Range: 0 to 24
EndMinute
Every day firmware update end time (minute). Range: 0 to 60
FileStatus
Firmware file status: create(1) -> new firmware file shall be stored on the device done(2) -> synchronization of storage device with MIB is done. Enumerations: create (1) done (2)
UploadResult
Firmware file upload result (error) code: success(1) -> the firmware file upload was successful, no-mem-card(2) -> no memory card plugged in, no-mem-space(3) -> no more space available on the memory card, incomp-fw-format(4) -> the firmware file format doesn't match the requirements, transfer-error(5) -> any transfer error occured during upload, write-protection(6) -> active write protection on storage device, internal-error(7) -> unexpected internal error occured. Enumerations: success (1) no-mem-card (2) no-mem-space (3) incomp-fw-format (4) transfer-error (5) write-protection (6) internal-error (7)

MIB Reference to Software Version 9.1.2 generated on 2012/09/25. Provided by webmaster@teldat.de Copyright ©2012 by Teldat GmbH