>> MIB - Management Information Base
>> Table: l2tpTunnelTable - (.1.3.6.1.4.1.272.4.23.8.30.10)
Description: Entries in this table are created by the system.
l2tpTunnelTable
OID | Name | Type | Access
.10 | RemoteIpAddress | IpAddress | R
.20 | RemoteUdpPort | INTEGER | R
.30 | RemoteTunnelId | INTEGER | R
.35 | RemoteReceiveWindowSize | INTEGER | R
.40 | RemoteHostname | DisplayString | R
.50 | RemoteVendorName | DisplayString | R
.60 | LocalIpAddress | IpAddress | R
.70 | LocalUdpPort | INTEGER | R
.80 | LocalTunnelId | INTEGER | R
.85 | LocalReceiveWindowSize | INTEGER | R
.90 | LocalHostname | DisplayString | R
.100 | Password | DisplayString | R
.120 | HelloInterval | INTEGER | RW
.130 | SessionDataSequencing | ENUM | RW
.140 | MinRetryTime | INTEGER | RW
.150 | MaxRetryTime | INTEGER | RW
.160 | MaxRetries | INTEGER | RW
.170 | State | ENUM | RW
RemoteIpAddress
The remote IP address for the tunnel.
RemoteUdpPort
The remote UDP port number for the tunnel. Range: 0 to 65535
RemoteTunnelId
The ID used by the remote end for the tunnel. Range: 0 to 65535
RemoteReceiveWindowSize
The receive window size used by L2TP on the remote side of this tunnel. Range: 1 to 65535
RemoteHostname
The name of the remote host. Length: 0 to 255
RemoteVendorName
The vendor name of the remote host L2TP layer. Length: 0 to 255
LocalIpAddress
The local IP address for the tunnel.
LocalUdpPort
The local UDP port number for the tunnel. Range: 0 to 65535
LocalTunnelId
The ID used by the local end for the tunnel. Range: 0 to 65535
LocalReceiveWindowSize
The receive window size used by L2TP on the local side of this tunnel. Currently, the only supported value is 1. Range: 1 to 1
LocalHostname
The name of the local host. Length: 0 to 255
Password
The password used for tunnel authentication. Length: 0 to 255
HelloInterval
The interval in seconds between two consecutive hello requests sent by L2TP during the tunnel life. If this object is set to 0 (zero), no hello requests are sent by L2TP on this tunnel. Range: 0 to 255
SessionDataSequencing
This object specifies if sequence numbers are used on the data channel of sessions supported by this tunnel. Enumerations: disabled (2) enabled (3)
MinRetryTime
The initial interval in seconds between two consecutive attempts to send an L2TP control packet. The value of this interval is doubled with each new attempt, until the maximum value defined in l2tpTunnelProfileMaxRetryTime is reached. Range: 1 to 255
MaxRetryTime
The maximum interval in seconds between two consecutive attempts to send an L2TP control packet. Range: 8 to 255
MaxRetries
The maximum number of retries to send an L2TP control packet. The total number of attempts will be one more than this value. Range: 1 to 255
State
The current state of the tunnel as specified in RFC2661. Selecting shutdown(5) value results in tunnel hangup. Any other value is ignored. Enumerations: idle (1) waitctlreply (2) waitctlconn (3) established (4) shutdown (5)

MIB Reference to Software Version 9.1.8 generated on 2014/07/15. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH