>> MIB - Management Information Base
>> Table: wlanBridge - (.1.3.6.1.4.1.272.4.46.12)
wlanBridge
OID | Name | Type | Access
.1 | ConfigScanTimeout | INTEGER | RW
.2 | ConfigSetupTimeout | INTEGER | RW
ConfigScanTimeout
This attribute defines the maximum time a bridge auto-configuration scan may take. After this timeout has expired, any auto-configuration scan will be aborted, regardless of current state. Range: 10 to 600
ConfigSetupTimeout
This attribute defines the maximum time a bridge auto-configuration setup may take. After this timeout has expired, any auto-configuration setup will be aborted, regardless of current state. In this case, artemBridgePeerConfigSetupResult will be set to 'timeout'. Range: 10 to 600

MIB Reference to Software Version 9.1.8 generated on 2014/07/15. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH