>> MIB - Management Information Base
>> Table: wlanStatisticsTable - (.1.3.6.1.4.1.272.4.46.14.1)
Description: Describe the WLAN statistics of a wlan card
wlanStatisticsTable
OID | Name | Type | Access
.1 | WlanIf | INTEGER | R
.2 | Operation | ENUM | RW
.10 | MSDUTxSuccess | Counter32 | R
.11 | MSDUTxMulti | Counter32 | R
.12 | MSDUTxDropped | Counter32 | R
.13 | MSDUTxFailed | Counter32 | R
.14 | MPDUTx | Counter32 | R
.15 | MPDUTxOneRetry | Counter32 | R
.16 | MPDUTxMultiRetry | Counter32 | R
.17 | MPDUTxFailed | Counter32 | R
.18 | MSDURxSuccess | Counter32 | R
.19 | MSDURxMulti | Counter32 | R
.20 | MSDURxDropped | Counter32 | R
.21 | MSDURxFailed | Counter32 | R
.22 | MPDURx | Counter32 | R
.23 | MPDURxDups | Counter32 | R
.24 | RTSSuccess | Counter32 | R
.25 | RTSFailed | Counter32 | R
.26 | ACKFailed | Counter32 | R
.27 | FramesRx | Counter32 | R
.28 | FrameRxError | Counter32 | R
.29 | FrameAborts | Counter32 | R
.30 | FrameAbortsPHY | Counter32 | R
.31 | PrivTxRejected | Counter32 | R
.32 | PrivRxPlain | Counter32 | R
.33 | PrivRxFailed | Counter32 | R
.34 | PrivRxNoKey | Counter32 | R
WlanIf
IfIndex of the wlan Interface the statistics belongs to.
Operation
Setting this variable to 'refresh' initiates a refresh of the statistic data. After refreshing it is autonomously changed to 'none'. Enumerations: none (1) refresh (2)
MSDUTxSuccess
The number of successfully transmitted unicast MSDUs.
MSDUTxMulti
The number of successfully transmitted multicast MSDUs.
MSDUTxDropped
The number of unicast and multicast MSDUs dropped before a transmission attempt was made.
MSDUTxFailed
The number of unicast and multicast MSDUs that could not be or were not successfully transmitted by the device.
MPDUTx
The number of successfully transmitted unicast and multicast MPDUs.
MPDUTxOneRetry
The number of unicast MPDUs successfully transmitted after one retry.
MPDUTxMultiRetry
The number of unicast MPDUs successfully transmitted after two or more retries.
MPDUTxFailed
The number of unicast MPDUs for which the maximum number of retries were exceeded.
MSDURxSuccess
The number of successfully received unicast MSDUs.
MSDURxMulti
The number of successfully received multicast MSDUs.
MSDURxDropped
The number of dropped unicast and multicast MSDUs.
MSDURxFailed
The number of partially or erroneously received unitcast and multicast MSDUs.
MPDURx
The number of successfully received unicast MPDUs.
MPDURxDups
The number of successfully received unicast MPDUs that were a duplicate of earlier frames.
RTSSuccess
The number of CTS frames received in response to an RTS frame.
RTSFailed
The number of transmitted RTS frames for which no response CTS frame was received.
ACKFailed
The object counts the number of frame transmissions for which an acknowledgment response frame was expected but not received.
FramesRx
The number of successfully received frames, before any address and type filtering.
FrameRxError
The number of unsuccessfully received frames.
FrameAborts
The number of aborted frames.
FrameAbortsPHY
The number of PHY aborted frames.
PrivTxRejected
The number of MPDUs that were not transmitted because no appropriate privacy configuration was available.
PrivRxPlain
The number of received MPDUs that were rejected because they were unencrypted.
PrivRxFailed
The number of received crypted MPDUs that were rejected because they could not be successfully decrypted.
PrivRxNoKey
The number of received crypted MPDUs that could not be decrypted because no key was available for decryption.

MIB Reference to Software Version 9.1.8 generated on 2014/07/15. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH