>> MIB - Management Information Base
>> Table: pppoeCreditsTable - (.1.3.6.1.4.1.272.4.24.2.1)
Description: The pppoeCreditsTable contains informations about current used resources and maximum allowed 'PPPoE-Service'-dependent resources. during a specified interval subsystem. Creating entries: Entries are added by the user. Deleting entries: Entries are removed by setting an entry's pppoeCreditsSurveillance object to 'delete'.
pppoeCreditsTable
OID | Name | Type | Access
.1 | Service | DisplayString | RW
.2 | Surveillance | ENUM | D
.3 | Measuretime | INTEGER | RW
.4 | MaxInCon | INTEGER | RW
.5 | MaxOutCon | INTEGER | RW
.6 | MaxInDuration | INTEGER | RW
.7 | MaxOutDuration | INTEGER | RW
.8 | Timeleft | INTEGER | RW
.9 | CurrentInCon | INTEGER | R
.10 | CurrentOutCon | INTEGER | R
.11 | TotalInCon | INTEGER | R
.12 | TotalOutCon | INTEGER | R
.13 | TotalInDuration | INTEGER | R
.14 | TotalOutDuration | INTEGER | R
.15 | CurrentAccount | INTEGER | R
Service
The PPPoE service name, indicating the service the Host is requesting. Length: 0 to 255
Surveillance
Surveillance on or off. Enumerations: off (1) on (2) delete (3)
Measuretime
Time of one observation interval in seconds.
MaxInCon
Maximum number of allowed incoming connections during the observation interval. -1 disables this limit.
MaxOutCon
Maximum number of allowed outgoing connections during the observation interval. -1 disables this limit.
MaxInDuration
Maximum connect time for incoming connections in seconds during the observation interval. -1 disables this limit.
MaxOutDuration
Maximum connect time for outgoing connections in seconds during the observation interval. -1 disables this limit
Timeleft
Time in seconds left in current interval. Writing to Timeleft will restart the observation interval.
CurrentInCon
Current number of incoming connections.
CurrentOutCon
Current number of outgoing connections.
TotalInCon
Total count of incoming connections during the observation interval.
TotalOutCon
Total count of outgoing connections during the observation interval.
TotalInDuration
Total connect time of incoming connections during the observation interval.
TotalOutDuration
Total connect time of outgoing connections during the observation interval.
CurrentAccount
Total connect time of all outgoing connections during the observation interval calculated in percent of 'pppoeCreditsMaxOutDuration'. Range: 0 to 100

MIB Reference to Software Version 9.1.8 generated on 2014/07/15. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH