>> MIB - Management Information Base
>> Table: capiPlciTable - (.1.3.6.1.4.1.272.4.7.3.1)
Description: The capiPlciTable contains information for each currently connected CAPI application (i.e. has a Physical Link Connection Identifier associated with it). Creating entries: Entries can only be made by the system. Upon receiving a CAPI_CONNECT_REQ (or CAPI_CONNECT_IND) message, the system assigns a unique PLCI (capiPlciNumber) and an entry is made. Deleting entries: Entries are automatically deleted by the system once a CAPI_DISCONNECT_RESP message is received.
capiPlciTable
OID | Name | Type | Access
.1 | Number | HexValue | R
.2 | Application | INTEGER | R
.3 | Controller | HexValue | R
.4 | State | ENUM | R
.5 | SelectB2Proto | ENUM | R
.6 | SelectB2Dlpd | OCTET STRING | R
.7 | SelectB3Proto | ENUM | R
.8 | SelectB3Ncpd | OCTET STRING | R
.9 | B1Proto | ENUM | R
.10 | B1Config | OCTET STRING | R
.11 | B2Proto | ENUM | R
.12 | B2Config | OCTET STRING | R
.13 | B3Proto | ENUM | R
.14 | B3Config | OCTET STRING | R
.15 | CipValue | INTEGER | R
.16 | InfoMask | HexValue | R
Number
The PLCI (physical link connection identifier) of the application. Range: 0 to -1
Application
The application-number (capiApplNumber).
Controller
The ISDN controller number. This value refers to the isdnStkNumber. Range: 0 to -1
State
The current link state as described in the CAPI state diagram. Enumerations: p-0 (1) p-1 (2) p-2 (3) p-3 (4) p-4 (5) p-5 (6) p-6 (7) p-7 (8) p-act (9)
SelectB2Proto
The current B2 protocol setting (CAPI 1.1 applications only). Enumerations: undef (1) x75 (2) hdlccrc (3) trans (4) sdlc (5) x75btx (6) fax (7) lapd (8) v110trans (9) v110sdlc (10) v110x75 (11) txonly (12) modem (241) v110sync (242)
SelectB2Dlpd
Current B2 protocol descriptor. DLPD = data link protocol descriptor (CAPI 1.1 applications only).
SelectB3Proto
Current B3 protocol setting (CAPI 1.1 applications only). Enumerations: undef (1) t70nl (2) iso8208 (3) t90 (4) trans (5) t30 (6)
SelectB3Ncpd
The current B3 Ncpd setting. NCPD = network control protocol descriptor (CAPI 1.1 applications only).
B1Proto
Current CAPI 2.0 B1 protocol setting. Enumerations: undef (1) hdlc (2) trans (3) v110trans (4) v110hdlc (5) faxg3 (6) hdlcinv (7) hdlc56 (8) modemneg (9) modemasync (10) modemsync (11)
B1Config
Current CAPI 2.0 B1 protocol configuration setting.
B2Proto
Current CAPI 2.0 B2 protocol setting. Enumerations: undef (1) x75 (2) trans (3) sdlc (4) lapd (5) t30 (6) ppp (7) transerr (8) modem (9)
B2Config
Current CAPI 2.0 B2 protocol configuration setting.
B3Proto
Current CAPI 2.0 B3 protocol setting. Enumerations: undef (1) trans (2) t90 (3) iso8208 (4) x25dce (5) t30 (6) t30ext (7) modem (9)
B3Config
Current CAPI 2.0 B3 protocol configuration setting.
CipValue
The current CIPValue setting.
InfoMask
The current InfoMask setting. Range: 0 to -1

MIB Reference to Software Version 9.1.8 generated on 2014/07/15. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH