>> MIB - Management Information Base
>> Table: mpsArsCarrierTable - (.1.3.6.1.4.1.272.4.53.10.6.1)
Description: This table contains information about carrier used by Automatic Route Selection feature.
mpsArsCarrierTable
OID | Name | Type | Access
.1 | Index | CarrierIndex | RW
.2 | DisplayName | DisplayString | RW
.3 | Number | DisplayString | RW
.4 | NumberPresentation | ENUM | RW
.5 | RoutingMode | ENUM | RW
.6 | RoutingModeNumber | DisplayString | RW
.7 | RoutingAdminStatus | ENUM | D
.8 | RoutingTargetIndex | INTEGER | RW
Index
A unique index for each carrier.
DisplayName
This object specifies a Carrier description for the Autom. Route Selection functionality. The DisplayName can be shown on the sytem phones. Length: 0 to 20
Number
This object specifies the number to be inserted to select a special route (carrier). Length: 0 to 12
NumberPresentation
show: number presentation is active (CLIP). hide: number presentation is restricted (CLIR). Enumerations: show (1) hide (2)
RoutingMode
This object specifies the routing mode for this carrier: RoutingMode=standard -> Route via standard (ClassOfService) settings, RoutingMode=bundle -> Route via selected trunk group/bundle table, RoutingMode=msn -> Route via selected MSN (e.g. internal GSM- Gateway). Enumerations: standard (1) bundle (2) msn (3)
RoutingModeNumber
This object specifies the bundle (number as string, reference to mpsTrunkBundleTable) or internal MSN depending on the selected RoutingMode. Length: 0 to 4
RoutingAdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)
RoutingTargetIndex
This variable contains the index (reference) of the target to be used for routing: RoutingMode=standard -> TargetIndex = 0, RoutingMode=bundle -> TargetIndex = mpsTrunkBundleIndex, RoutingMode=msn -> TargetIndex = mpsExtensionIndex.

MIB Reference to Software Version 9.1.8 generated on 2014/07/15. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH