>> MIB - Management Information Base
>> Table: dot11HTStationConfigTable - (.1.2.840.10036.1.16.1)
Description: An entry (conceptual row) in the dot11HTStationConfig Table. ifIndex - Each IEEE 802.11 interface is represented by an ifEntry. Interface tables in this MIB module are indexed by ifIndex.
dot11HTStationConfigTable
OID | Name | Type | Access
.1 | HTOperationalMCSSet | OCTET STRING | RW
.2 | MIMOPowerSave | ENUM | R
.3 | NDelayedBlockAckOptionImplemented | ENUM | R
.4 | MaxAMSDULength | INTEGER | R
.5 | PSMPOptionImplemented | ENUM | R
.6 | STBCControlFrameOptionImplemented | ENUM | R
.7 | LsigTxopProtectionOptionImplemented | ENUM | R
.8 | MaxRxAMPDUFactor | INTEGER | R
.9 | MinimumMPDUStartSpacing | INTEGER | R
.10 | PCOOptionImplemented | ENUM | R
.11 | TransitionTime | INTEGER | R
.12 | MCSFeedbackOptionImplemented | ENUM | R
.13 | HTControlFieldSupported | ENUM | R
.14 | RDResponderOptionImplemented | ENUM | R
HTOperationalMCSSet
This attribute shall specify the set of MCS at which the station may transmit data. Each octet contains a value representing a rate. Each MCS shall be within the range from 1 to 127, and shall be supported for receiving data. This value is reported in transmitted Beacon, Probe Request, Probe Response, Association Request, Association Response, Reassociation Request, and Reassociation Response frames, and is used to determine whether a BSS with which the station desires to synchronize is suitable. It is also used when starting a BSS, as specified in 10.3. Length: 1 to 127
MIMOPowerSave
This is an 8-bit integer value that identifies the configured power save state of MIMO. Enumerations: static (1) dynamic (2) mimo (3)
NDelayedBlockAckOptionImplemented
This attribute, when TRUE, indicates that the station implementation is capable of supporting the No ack option of the Delayed Block Ack. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
MaxAMSDULength
This attribute indicates the supported maximum size of AMSDU. The default value of this attribute is 3839. Range: 3839 to 7935
PSMPOptionImplemented
This attribute, when TRUE, indicates that the station implementation is capable of supporting PSMP. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
STBCControlFrameOptionImplemented
This attribute, when TRUE, indicates that the station implementation is capable of processing the received control frames that are STBC frames. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
LsigTxopProtectionOptionImplemented
This attribute, when TRUE, indicates that the station implementation is capable of supporting L-SIG TXOP Protection option. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
MaxRxAMPDUFactor
This attribute indicates the maximum length of A-MPDU that the STA can receive. The Maximum Rx A-MPDU defined by this field is equal to 213+dot11MaxRxAMPDUFactor -1 octets. The default value of this attribute is 0. Range: 0 to 3
MinimumMPDUStartSpacing
This attribute indicates the minimum time between the start of adjacent MPDUs within an A-MPDU. This time is measured at the PHY-SAP; the number of octets between the start of two consecutive MPDUs in A-MPDU shall be equal or greater than (dot11MinimumMPDUStartSpacing*PHY-bit-rate)/8. The encoding of the minimum time to this attribute is: 0 no restriction 1 1/4 microsec 2 1/2 microsec 3 1 microsec 4 2 microsec 5 4 microsec 6 8 microsec 7 16 microsec The default value of this attribute is 0. Range: 0 to 7
PCOOptionImplemented
This attribute, when TRUE, indicates that the station implementation is capable of supporting Phased Coexistence Operation. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
TransitionTime
This attribute indicates that the minimum transition time within which the STA can switch between 20 MHz channel width and 40 MHz channel width with a high probability. The encoding of the transition time to this attribute is: 400 microsec 1500 microsec 5000 microsec The default value of this attribute is 3. Range: 1 to 3
MCSFeedbackOptionImplemented
This attribute indicates the MCS feed back capability supported by the station implementation. The default value of this attribute is 0. Enumerations: none (0) unsolicited (2) both (3)
HTControlFieldSupported
This attribute, when TRUE, indicates that the station implementation is capable of receiving HT Control field. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
RDResponderOptionImplemented
This attribute, when TRUE, indicates that the station implementation is capable operating as a RD responder. The default value of this attribute is FALSE. Enumerations: true (1) false (2)

MIB Reference to Software Version 9.1.8 generated on 2014/07/15. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH