>> MIB - Management Information Base
>> Table: systemPhoneFwuProcessTable - (.1.3.6.1.4.1.272.4.64.5.3.1)
Description: This table contains information of firmware update of system phones.
systemPhoneFwuProcessTable
OID | Name | Type | Access
.1 | Index | SystelTerminalIndex | RW
.2 | StartNow | ENUM | RW
.3 | StartSchedule | ENUM | RW
.4 | Status | ENUM | R
.5 | Result | ENUM | R
.6 | Progress | INTEGER | R
.7 | UnknownMsgCounter | Unsigned32 | R
.8 | TimeoutCounter | Unsigned32 | R
.9 | AdminStatus | ENUM | D
Index
A reference to the systemPhoneTable (or mpsTerminalTable). Range: 1 to 65535
StartNow
This variable contains the user input in a boolean value to immediately update the firmware of this device. Enumerations: true (1) false (2)
StartSchedule
If this variable is true, the firmwareupdate starts scheduled. The period of firmware updates is defined in systemPhoneFwuServerTable. Enumerations: true (1) false (2)
Status
Status of system phone firmware update: done: there is no firmware update in time running: firmwareupdate is actually running waiting: because lack of system ressources the scheduled or immediately started firmware update is in waiting mode. Enumerations: done (1) running (2) waiting (3)
Result
Result of system phone firmware update: idle: initial value ok: firmware update is successfully completed failed: an error occurred during the firmware update process. Enumerations: idle (1) ok (2) failed (3)
Progress
Progress of system phone firmware update. Range: 0 to 100
UnknownMsgCounter
Statistic value which shows the received unknown messages of internal firmware download server during the firmware update.
TimeoutCounter
Statistic value which shows the occured timeouts during the firmware update.
AdminStatus
In case of elmegIP (gigaset) devices this variable activates (enable) or deactivates (disable) the automatic update function of gigaset devices (introduced by a SIP NOTIFY check-sync). Other systemphones ignore the AdminStatus-value. To delete this mib, value must be set to delete. Enumerations: enable (1) delete (2) disable (3)

MIB Reference to Software Version 9.1.8 generated on 2014/07/15. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH