>> MIB - Management Information Base
>> Table: wlcWTPMaintenanceTable - (.1.3.6.1.4.1.272.4.61.1.4.1)
Description: This table delivers maintenance/debugging actions executed on the WTP
wlcWTPMaintenanceTable
OID | Name | Type | Access
.1 | Index | INTEGER | RW
.2 | State | ENUM | D
.3 | Command | ENUM | RW
.4 | URL | DisplayString | RW
Index
Index of WTP to be addressed with maintenance command.
State
This variable displays the current maintenance state of each WTP: idle: idle state start: start maintenance event (get state file or do update) running: maintenance event is running rebooting: WTP is rebooting with new image, done: maintenance event successfully finished error: an error occured, stopped: WTP already has the image version delete: delete maintenance event. Enumerations: idle (1) start (2) running (3) done (4) error (5) stopped (6) rebooting (7) delete (32)
Command
Type of action performed on WTP software: software update state: get state file Enumerations: state (1) software (2)
URL
Contains URL of the http or tftp server. Depending on wlcWTPMaintenanceCommand it serves for either destination (command state) or source (command software). Length: 0 to 255

MIB Reference to Software Version 9.1.8 generated on 2014/07/15. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH