>> MIB - Management Information Base
>> Table: vmsGlobalAdm - (.1.3.6.1.4.1.272.4.34.1.1)
vmsGlobalAdm
OID | Name | Type | Access
.1 | Status | ENUM | RW
.2 | AccountRef | INTEGER | RW
.3 | SipPort | INTEGER | RW
.4 | Language | ENUM | RW
.5 | SmtpServer | DisplayString | RW
.6 | SmtpPort | INTEGER | RW
.7 | SmtpFrom | DisplayString | RW
.8 | SmtpUser | DisplayString | RW
.9 | SmtpPassword | DisplayString | RW
.10 | FileAdminStatus | ENUM | RW
.11 | FileOperStatus | ENUM | R
.12 | MaxLifeTime | INTEGER | RW
Status
Activate or deactivate the voice mail system. Enumerations: enabled (1) disabled (2)
AccountRef
This value contains the reference to the account number of the Voice Mail Server. Reference to mpsExtensionIndex in mpsExtensionTable.
SipPort
UDP port number used for (system internal) SIP connect. Range: 1 to 65535
Language
The global language setting for the voice mail server. Enumerations: german (1) dutch (2) english (3) italian (5) french (10)
SmtpServer
The IP address of the SMTP server. This object may contain either an IP address or a domain name. Length: 0 to 255
SmtpPort
The TCP port to be used in order to connect to vmsGlobSmtpServer.
SmtpFrom
Sender adress, e.g. voicemail@thecompany.com. Length: 0 to 255
SmtpUser
SMTP account/user name. Length: 0 to 255
SmtpPassword
SMTP password. Length: 0 to 255
FileAdminStatus
File admin status: idle(1) : no action create(2): new wave files shall be stored on the storage device remove(3): files shall be deleted on the storage device Enumerations: idle (1) create (2) remove (3)
FileOperStatus
File oper status: unavailable(1): Ann. wave files not yet available on the storage device inProgress(2) : Create or remove file just in progress available(3) : synchronization of storage device with MIB is done. Enumerations: unavailable (1) inProgress (2) available (3)
MaxLifeTime
Maximum life time of messages in days. After this time a message can be displaced by a new message. Range: 10 to 60

MIB Reference to Software Version 9.1.8 generated on 2014/07/15. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH