>> MIB - Management Information Base
>> Table: tr069InformEventTable - (.1.3.6.1.4.1.272.4.22.6.4.1.1)
Description: Table of pending TR069 Inform events
tr069InformEventTable
OID | Name | Type | Access
.1 | Code | ENUM | RW
.2 | Name | DisplayString | RW
.3 | Time | INTEGER | RW
.4 | CommandKey | DisplayString | RW
Code
Type of the event. Enumerations: bootstrap (1) boot (2) periodic (3) scheduled (4) valuechange (5) kicked (6) connectionrequest (7) transfercomplete (8) diagnosticscomplete (9) requestdownload (10) methodinduced (11) vendorspecific (12)
Name
This is transmitted as EventCode (see spec). Only necessary for EventTypes 9 & 10 Length: 0 to 32
Time
Absolute time (time_t localtime) the event is scheduled to fire. 0 means ASAP
CommandKey
Opaque value proivded by the ACS Length: 0 to 32

MIB Reference to Software Version 9.1.8 generated on 2014/07/15. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH