>> MIB - Management Information Base
>> Table: pppSessionTable - (.1.3.6.1.4.1.272.4.3.10.1)
Description: The pppSessionTable contains statistical information for the PPP protocol. Only the system can add or delete entries to this table. Creating entries: Entries are created by the system each time a new PPP connection is created. Deleting entries: Entries are removed by the system when the corresponding PPP connection is terminated.
pppSessionTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | R
.2 | Mlp | ENUM | R
.3 | Mru | Counter | R
.4 | LcpCallback | ENUM | R
.5 | AuthProt | ENUM | R
.6 | Compression | ENUM | R
.7 | Encryption | ENUM | R
.8 | CbcpMode | ENUM | R
.9 | CbcpDelay | INTEGER | R
.10 | LocIpAddr | IpAddress | R
.11 | RemIpAddr | IpAddress | R
.12 | DNS1 | IpAddress | R
.13 | DNS2 | IpAddress | R
.14 | WINS1 | IpAddress | R
.15 | WINS2 | IpAddress | R
.16 | VJHeaderComp | ENUM | R
.18 | BacpFavoredPeer | ENUM | R
.19 | IpcpStatus | ENUM | R
.20 | Ipcp6Status | ENUM | R
.21 | Ipcp6LocIfId | OCTET STRING | R
.22 | Ipcp6RemIfId | OCTET STRING | R
IfIndex
Correlating PPP interface index.
Mlp
Indicates negotiation of Multilink PPP. Enumerations: none (1) negotiated (2)
Mru
Peer's MRU/MRRU LCP option.
LcpCallback
Callback option inside LCP negotiation. Enumerations: none (1) lcp (2) cbcp (3)
AuthProt
The negotiated PPP authentication protocol. Enumerations: none (1) pap (2) chap (3) ms-chapv1 (4) ms-chapv2 (5)
Compression
The negotiated CCP compression mode. Enumerations: none (1) stac (2) ms-stac (3) mppc (4)
Encryption
The negotiated CCP encryption mode. Enumerations: none (1) mppe-40 (2) mppe-128 (3) des-56 (4) triple-des-168 (5) blowfish-168 (6) mppe-56 (7) mppev2-40 (8) mppev2-56 (9) mppev2-128 (10) blowfish-56 (11) mppev2-40-rfc3078 (12) mppev2-56-rfc3078 (13) mppev2-128-rfc3078 (14)
CbcpMode
The negotiated Callback Control Protocol (CBCP) mode. Enumerations: none (1) no-callback (2) user-specified (3) pre-specified (4)
CbcpDelay
The negotiated (CBCP) callback delay in seconds. Range: 0 to 60
LocIpAddr
The negotiated local IP Address.
RemIpAddr
The negotiated remote IP Address.
DNS1
The negotiated first name server IP address.
DNS2
The negotiated second name server IP address.
WINS1
The negotiated first NetBIOS name server (WINS) IP address.
WINS2
The negotiated second NetBIOS name server (WINS) IP address.
VJHeaderComp
The negotiation of Van Jacobsen TCP/IP header compression option (IPCP). Enumerations: none (1) negotiated (2)
BacpFavoredPeer
The result of the BACP Favored-Peer negotiation. Enumerations: none (1) local (2) remote (3)
IpcpStatus
IPCP FSM status according RFC 1548. Enumerations: initial (1) starting (2) closed (3) stopped (4) closing (5) stopping (6) reqsent (7) ackrcvd (8) acksent (9) opened (10)
Ipcp6Status
IPCP6 FSM status according RFC i1548 and 2472.
Ipcp6LocIfId
The negotiated local IPCP6 interface ID.
Ipcp6RemIfId
The negotiated remote IPCP6 interface ID.

MIB Reference to Software Version 9.1.8 generated on 2014/07/15. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH