>> MIB - Management Information Base
>> Table: ipMRouteInterfaceTable - (.1.3.6.1.2.1.83.1.1.4.1)
Description: An entry (conceptual row) containing the multicast routing information for a particular interface.
ipMRouteInterfaceTable
OID | Name | Type | Access
.1 | IfIndex | InterfaceIndex | R
.2 | Ttl | Integer32 | RW
.3 | Protocol | ENUM | R
.4 | RateLimit | Integer32 | RW
.5 | InMcastOctets | Counter32 | R
.6 | OutMcastOctets | Counter32 | R
.7 | HCInMcastOctets | Counter64 | R
.8 | HCOutMcastOctets | Counter64 | R
IfIndex
The ifIndex value of the interface for which this entry contains information. Range: 1 to 2147483647
Ttl
The datagram TTL threshold for the interface. Any IP multicast datagrams with a TTL less than this threshold will not be forwarded out the interface. The default value of 0 means all multicast packets are forwarded out the interface. Range: 0 to 255
Protocol
The routing protocol running on this interface. Enumerations: other (1) local (2) netmgmt (3) dvmrp (4) mospf (5) pimSparseDense (6) cbt (7) pimSparseMode (8) pimDenseMode (9) igmpOnly (10) bgmp (11) msdp (12)
RateLimit
The rate-limit, in kilobits per second, of forwarded multicast traffic on the interface. A rate-limit of 0 indicates that no rate limiting is done.
InMcastOctets
The number of octets of multicast packets that have arrived on the interface, including framing characters. This object is similar to ifInOctets in the Interfaces MIB, except that only multicast packets are counted.
OutMcastOctets
The number of octets of multicast packets that have been sent on the interface.
HCInMcastOctets
The number of octets of multicast packets that have arrived on the interface, including framing characters. This object is a 64-bit version of ipMRouteInterfaceInMcastOctets. It is similar to ifHCInOctets in the Interfaces MIB, except that only multicast packets are counted.
HCOutMcastOctets
The number of octets of multicast packets that have been sent on the interface. This object is a 64-bit version of ipMRouteInterfaceOutMcastOctets.

MIB Reference to Software Version 9.1.8 generated on 2014/07/15. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH