>> MIB - Management Information Base
>> Table: mpsTrunkNumberTable - (.1.3.6.1.4.1.272.4.53.3.7.1)
Description: This table contains advanced information about external numbers.
mpsTrunkNumberTable
OID | Name | Type | Access
.1 | Index | TrunkNumberIndex | RW
.2 | Group | TrunkGroupIndexOrZero | RW
.3 | NumberIndex | Unsigned32 | RW
.4 | Type | ENUM | RW
.5 | Target | ENUM | RW
.6 | TargetIndex | INTEGER | RW
.7 | NumberEntry | DisplayString | RW
.8 | Calendar | CalendarIndexOrZero | RW
.9 | DisplayName | DisplayString | RW
.10 | AdminStatus | ENUM | D
.11 | ReRouteAppl | ReRouteApplIndexOrZero | RW
Index
A unique value for each trunk number. Range: 1 to 65535
Group
A unique value for each trunk group index. 0 allowed for mpsTrunkNumberType = cnsIndividual, for all trunk groups Range: 0 to 65535
NumberIndex
A unique value for each number entry of a trunk group.
Type
This variable contains the information of the type of number: msn : MSN ddi : DDI (direct dialling in) cnsIndividual : clip no screening additionalMSN : MSN at point-to-point device Enumerations: msn (1) ddi (2) cnsIndividual (3) additionalMSN (4)
Target
The external number can be assigned to an internal target: group: a group of internal extensions. extension: one internal extension. call-through: use the call-through feature re-route: direct routing to announcement telematicAccess: telematic control isdnLogin: console login webServiceLogin: web access call-center: group call center Enumerations: group (1) extension (2) call-through (3) re-route (4) telematicAccess (5) isdnLogin (6) webServiceLogin (7) call-center (8)
TargetIndex
This variable contains index of the target table or zero, mpsTrunkNumberTarget=group : index = mpsGroupIndex. mpsTrunkNumberTarget=extension : index = ExtensionIndex. mpsTrunkNumberTarget=call-center : index = mpsGroupIndex (call-center) for all other set to 0.
NumberEntry
This variable contains the digits of the external number (MSN,DDI,...). Length: 0 to 24
Calendar
Select a calendar index to switch the call distribution for immediately rerouting automatically. Range: 0 to 65535
DisplayName
Display name of the trunk number. Length: 0 to 32
AdminStatus
Just for MIB entry deletion. Enumerations: enable (1) delete (2)
ReRouteAppl
Index of ReRouting application in mpsReRouteApplTable. Value 0 means that ReRouting application is inactive. Range: 0 to 65535

MIB Reference to Software Version 9.1.8 generated on 2014/07/15. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH