>> MIB - Management Information Base
>> Table: ipSessionTable - (.1.3.6.1.4.1.272.4.5.7.1)
Description: .
ipSessionTable
OID | Name | Type | Access
.1 | SrcAddr | IpAddress | R
.2 | SrcPort | INTEGER | R
.3 | DstAddr | IpAddress | R
.4 | DstPort | INTEGER | R
.5 | OutPkts | Counter32 | R
.6 | OutOctets | Counter32 | R
.7 | InPkts | Counter32 | R
.8 | InOctets | Counter32 | R
.9 | Protocol | ENUM | R
.10 | Age | TimeTicks | R
.11 | Idle | TimeTicks | R
.12 | SrcIfIndex | INTEGER | R
.13 | DstIfIndex | INTEGER | R
SrcAddr
source address of IP session
SrcPort
source port of IP session Range: 0 to 65535
DstAddr
destination port of IP session
DstPort
destination port of IP session Range: 0 to 65535
OutPkts
outgoing packets in IP session
OutOctets
outgoing octets in IP session
InPkts
incoming packets in IP session
InOctets
incoming octets in IP session
Protocol
protocol of IP session Enumerations: icmp (1) igmp (2) ggp (3) tcp (6) egp (8) pup (12) udp (17) hmp (20) xns-idp (22) rdp (27) ipv6 (41) rsvp (46) gre (47) esp (50) ah (51) igrp (88) ospf (89) pim (103) l2tp (115) reserved (255)
Age
age of IP session
Idle
idle time of IP session
SrcIfIndex
source interface index of IP session
DstIfIndex
destination interface index of IP session

MIB Reference to Software Version 9.1.8 generated on 2014/07/15. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH