>> MIB - Management Information Base
>> Table: mpsTerminalTable - (.1.3.6.1.4.1.272.4.53.14.1.1)
Description: This table contains information about terminal endpoints.
mpsTerminalTable
OID | Name | Type | Access
.1 | Index | TerminalIndex | RW
.2 | IfIndex | InterfaceIndexOrZero | RW
.3 | PhoneType | ENUM | RW
.4 | Type | ENUM | RW
.5 | Descr | DisplayString | RW
.6 | AdminStatus | ENUM | D
.7 | DoorIntercom | DoorIntercomIndexOrZero | RW
.8 | IPSystelPort | INTEGER | R
.9 | InterfaceType | ENUM | RW
.10 | OperStatus | ENUM | R
.11 | MacAddress | MacAddress | RW
.12 | OEMType | ENUM | RW
Index
A unique value for each terminal. Range: 1 to 65535
IfIndex
Reference to mpsDeviceTable. 0 = no reference. Range: 0 to 2147483647
PhoneType
Select the phone type of the terminal: standard (1) : standard terminal systemphone (2) : the terminal is a system phone vms (3) : internal Voice Mail Server oem-phone (4) : the terminal is a OEM phone. Enumerations: standard (1) systemphone (2) vms (3) oem-phone (4)
Type
This varibale contains the terminal type: telephone(1) : 'normal' phone answering-machine(2): answering machine voice-mail(3) : external voice mail server ermergency-phone(4) : allow ermergency calls with high priority Enumerations: telephone (1) answering-machine (2) voice-mail (3) emergency-phone (4)
Descr
A textual description of the terminal endpoint. Length: 0 to 20
AdminStatus
Admin status of the terminal. Set to 'delete' to delete the whole entry. Enumerations: enable (1) delete (2) disable (3)
DoorIntercom
This variable contains the number of the door intercom, refer to mpsDoorIntercomIndex in mpsDoorIntercomTable, only valid for mpsTerminalPhoneType = standard and mpsTerminalType = telephone. Range: 0 to 10
IPSystelPort
This variable contains the RTP port number for IP system phone.
InterfaceType
This variable contains the interface type, for which type of interface this terminal can be used. Enumerations: isdn (1) voip (2) pots (3)
OperStatus
Operational status of the terminal. Enumerations: up (1) down (2) licMissing (3)
MacAddress
This variable contains the MAC address of the IP terminal. Length: 6 to 6
OEMType
OEM device type of the terminal e.g. Siemens OpenStage, Gigaset... Enumerations: none (1) openstage (2) gigaset (3)

MIB Reference to Software Version 9.1.8 generated on 2014/07/15. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH