>> MIB - Management Information Base
>> Table: ipDynAddrPoolTable - (.1.3.6.1.4.1.272.4.5.52.4.1)
Description: This table defines all dynamic IP address pools of the system. Pools don't have to overlap in their ip address range. Corrections therefor are made autonomous by the system. Pools can be shared amongst subsystems/ user types.
ipDynAddrPoolTable
OID | Name | Type | Access
.1 | Identifier | DynIpPoolId | RW
.2 | Description | DisplayString | RW
.3 | FirstAddr | IpAddress | RW
.4 | Range | INTEGER | RW
.5 | DnsServer1 | IpAddress | RW
.6 | DnsServer2 | IpAddress | RW
.7 | AdminStatus | ENUM | D
Identifier
This object uniquely identifies the dynamic IP address pool in the system. Range: 0 to 65535
Description
The name of the pool, only used for descriptive purposes (max. 50 characters). Length: 0 to 50
FirstAddr
The first IP address of the pool. A value of 0.0.0.0 disables the pool.
Range
The number of consequtive IP addresses available in this pool starting with (and including) ipDynAddrPoolFirstAddr. A value of 0 disables the pool. Note that when the range is truncated by setting a smaller range or a 'higher' ipDynAddrPoolFirstAddr, the related entries in the ipDynaAddrTable which are not covered any longer by this pool are autonomous removed by the system. Range: 0 to 16777214
DnsServer1
This object specifies the Primary Domain Name Server to be given to the client via 'domain name server option'. If either ipStatAddrDnsServer1 or ipStatAddrDnsServer2 value is assigned (i.e. is not 255.255.255.255), ipDynAddrPoolDnsServer1 and ipDynAddrPoolDnsServer2 are ignored in favor of these parameters. If both ipDynAddrPoolDnsServer1 and ipDynAddrPoolDnsServer2 are assigned 0.0.0.0 the Primary and Secondary DNS IP addresses are chosen according to setting of variable ipDnsDhcpAssign and optionally contents of ipDnsServerOper MIB table. See description of these objects for details.
DnsServer2
This object specifies the Secondary Domain Name Server to be given to the client via 'domain name server option'. If either ipStatAddrDnsServer1 or ipStatAddrDnsServer2 value is assigned (i.e. is not 255.255.255.255), ipDynAddrPoolDnsServer1 and ipDynAddrPoolDnsServer2 are ignored in favor of these parameters. If both ipDynAddrPoolDnsServer1 and ipDynAddrPoolDnsServer2 are assigned 0.0.0.0 the Primary and Secondary DNS IP addresses are chosen according to setting of variable ipDnsDhcpAssign and optionally contents of ipDnsServerOper MIB table. See description of these objects for details.
AdminStatus
MIB entry deletion is performed by this object: - enable : enables ipDynAddrPoolTable entry - delete : deletes ipDynAddrPoolTable entry. Enumerations: enable (1) delete (2)

MIB Reference to Software Version 9.1.8 generated on 2014/07/15. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH