>> MIB - Management Information Base
>> Table: dot11RegDomainsSupportedTable - (.1.2.840.10036.4.7.1)
Description: An entry in the dot11RegDomainsSupport Table. ifIndex - Each 802.11 interface is represented by an ifEntry. Interface tables in this MIB module are indexed by ifIndex.
dot11RegDomainsSupportedTable
OID | Name | Type | Access
.1 | Index | Integer32 | R
.2 | Value | ENUM | R
Index
The auxiliary variable used to identify instances of the columnar objects in the RegDomainsSupport Table. Range: 1 to 2147483647
Value
There are different operational requirements dependent on the regulatory domain. This attribute list describes the regulatory domains the PLCP and PMD support in this implementation. Currently de- fined values and their corresponding Regulatory Domains are: FCC (USA) = X'10', DOC (Canada) = X'20', ETSI (most of Europe) = X'30', Spain = X'31', France = X'32', MKK (Japan) = X'40' Enumerations: fcc (16) doc (32) etsi (48) spain (49) france (50) mkk (64)

MIB Reference to Software Version 9.1.8 generated on 2014/07/15. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH