>> MIB - Management Information Base
>> Table: wlanACLTable - (.1.3.6.1.4.1.272.4.46.8.1)
Description: The WLAN Access List based on MAC Addresses
wlanACLTable
OID | Name | Type | Access
.1 | Address | MacAddress | RW
.2 | IfIndex | INTEGER | RW
.3 | Status | ENUM | D
Address
The MAC Address for the accepted client Length: 6 to 6
IfIndex
The VSS Interface the MAC Address belongs
Status
The Status for the entry (delete) Enumerations: enable (1) disable (2) delete (3)

MIB Reference to Software Version 9.1.8 generated on 2014/07/15. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH