>> MIB - Management Information Base
>> Table: ipDnsStaticTable - (.1.3.6.1.4.1.272.4.5.20.18.1)
Description: Contains administrative (static) DNS-entries. Three different entry-types are allowed. 1) 'Positive' entries store names and addresses for building related A/AAAA/PTR-resource-records. 2) 'Negative' (and 'ignore') entries store 'invalid' names for rejecting (or ignoring) related queries/questions. 3) 'Wildcard' entries store name-patterns and nameserver- interfaces/addresses for forwarding related queries.
ipDnsStaticTable
OID | Name | Type | Access
.1 | Index | INTEGER | RW
.2 | Name | DisplayString | RW
.3 | IpaddrType | ENUM | RW
.4 | Ipaddr | InetAddress | RW
.5 | Response | ENUM | D
.6 | IfIndex | INTEGER | RW
.7 | NameServerAddrType | ENUM | RW
.8 | NameServerAddr | InetAddress | RW
.9 | NameServ2AddrType | ENUM | RW
.10 | NameServ2Addr | InetAddress | RW
.11 | FullName | DisplayString | R
.12 | Hash | INTEGER | R
Index
Unique index for unambiguous SNMP-addressing, automatically updated to next free/unused value if initialised to 0.
Name
For 'wildcard' entries, specifies name-pattern with leading '*.' substring. (Any further '*' characters in pattern have NO special meaning.) Entry matches if no other (more specific) cache-entries match and if query/question-name is equal to or sub-domain of specified name-pattern. For all other entries, specifies related DNS-name. If contains dots then is treated as full domain-names. Otherwise is treated as simple name to be extended by globally configured domain-name from admin-table. For any entries (wildcard or not), name is automatically copied to 'FullName' field and completed there (i.e. top-domain added for simple names, missing trailing dots added for any names). Length: 0 to 255
IpaddrType
IP-version for ipDnsStaticEntIpaddr. Must be ipv4 or ipv6. Relevant only for 'positive' non-wildcard entries. Remark: Values 'unknown', 'ipv4z', 'ipv6z', 'dns' are inherited from InetAddressType but are NOT allowed here. Enumerations: unknown (0) ipv4 (1) ipv6 (2) ipv4z (3) ipv6z (4) dns (16)
Ipaddr
IPv4/IPv6-address to be used for name/address-resolution. Relevant only for 'positive' non-wildcard entries. Length: 0 to 255
Response
Field serves multiple purposes. 'delete' means that entry shall be removed. Any other value specifies entry-type. 'ignore'/'negative' means that queries for specified name shall be ignored/rejected. 'positive' means that entry is either 'normal' cache-entry or wildcard (if name starts with '*.'). Normal entries store name and address for building related A/AAAA/PTR-resource-records, and wildcards are used for forwarding queries for certain domains and their sub-domains to other nameservers. Enumerations: ignore (1) negative (2) positive (3) delete (4)
IfIndex
Relevant only for wildcard-entries with DHCP/IPCP-assigned nameservers (i.e. address not known at configuration-time). Should be set to -1 (unspecified) otherwise. Tells interface-index of nameserver-entry for forwarding matching queries/questions. If wildcard-entry does NOT specify nameservers (neither by address nor by interface) then matching queries are forwarded to ANY nameservers from global table.
NameServerAddrType
IP-version for ipDnsStaticEntNameServerAddr. Must be ipv4 (IPv6-transport not yet supported). Relevant only for wildcard-entries with statically configured nameservers. Remark: Values 'unknown', 'ipv6', 'ipv4z', 'ipv6z', 'dns' are inherited from InetAddressType but are NOT allowed here. Enumerations: unknown (0) ipv4 (1) ipv6 (2) ipv4z (3) ipv6z (4) dns (16)
NameServerAddr
Relevant only for wildcard-entries with statically configured nameservers. Should be set to 0 (unspecified) otherwise. Tells IPv4-address of primary nameserver for forwarding matching queries. If wildcard-entry does NOT specify nameservers (neither by address nor by interface) then matching queries are forwarded to ANY nameservers from global table. Length: 0 to 255
NameServ2AddrType
IP-version for ipDnsStaticEntNameServ2Addr. Must be ipv4 (IPv6-transport not yet supported). Relevant only for wildcard-entries with statically configured nameservers. Remark: Values 'unknown', 'ipv6', 'ipv4z', 'ipv6z', 'dns' are inherited from InetAddressType but are NOT allowed here. Enumerations: unknown (0) ipv4 (1) ipv6 (2) ipv4z (3) ipv6z (4) dns (16)
NameServ2Addr
Relevant only for wildcard-entries with statically configured nameservers. Should be set to 0 (unspecified) otherwise. Tells IPv4-address of secondary nameserver for forwarding matching queries. Length: 0 to 255
FullName
Automatically generated: Full DNS-name or name-pattern, derived from administrative 'Name' field. Length: 0 to 255
Hash
Automatically generated: Hash-value of name-field. Relevant only for non-wildcard-entries.

MIB Reference to Software Version 9.1.8 generated on 2014/07/15. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH