>> MIB - Management Information Base
>> Table: system - (.1.3.6.1.2.1.1)
system
OID | Name | Type | Access
.1 | Descr | DisplayString | RW
.2 | ObjectID | OBJECT IDENTIFIER | R
.3 | UpTime | TimeTicks | R
.4 | Contact | DisplayString | RW
.5 | Name | DisplayString | RW
.6 | Location | DisplayString | RW
.7 | Services | INTEGER | R
Descr
A textual description of the entity. This value should include the full name and version identification of the system's hardware type, software operating-system, and networking software. Length: 0 to 255
ObjectID
The vendor's authoritative identification of the network management subsystem contained in the entity. This value is allocated within the SMI enterprises subtree (1.3.6.1.4.1) and provides an easy and unambiguous means for determining `what kind of box' is being managed. For example, if vendor `Flintstones, Inc.' was assigned the subtree 1.3.6.1.4.1.424242, it could assign the identifier 1.3.6.1.4.1.424242.1.1 to its `Fred Router'.
UpTime
The time (in hundredths of a second) since the network management portion of the system was last re-initialized.
Contact
The textual identification of the contact person for this managed node, together with information on how to contact this person. If no contact information is known, the value is the zero-length string. Length: 0 to 255
Name
An administratively-assigned name for this managed node. By convention, this is the node's fully-qualified domain name. If the name is unknown, the value is the zero-length string. Length: 0 to 255
Location
The physical location of this node (e.g., 'telephone closet, 3rd floor'). If the location is unknown, the value is the zero-length string. Length: 0 to 255
Services
A value which indicates the set of services that this entity may potentially offer. The value is a sum. This sum initially takes the value zero. Then, for each layer, L, in the range 1 through 7, that this node performs transactions for, 2 raised to (L - 1) is added to the sum. For example, a node which performs only routing functions would have a value of 4 (2^(3-1)). In contrast, a node which is a host offering application services would have a value of 72 (2^(4-1) + 2^(7-1)). Note that in the context of the Internet suite of protocols, values should be calculated accordingly: layer functionality 1 physical (e.g., repeaters) 2 datalink/subnetwork (e.g., bridges) 3 internet (e.g., supports the IP) 4 end-to-end (e.g., supports the TCP) 7 applications (e.g., supports the SMTP) For systems including OSI protocols, layers 5 and 6 may also be counted. Range: 0 to 127

MIB Reference to Software Version 9.1.9 generated on 2014/07/17. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH