>> MIB - Management Information Base
>> Table: dot11TxBFConfigTable - (.1.2.840.10036.4.18.1)
Description: An entry in the dot11TxBFConfig Table. ifIndex - Each 802.11 interface is represented by an ifEntry. Interface tables in this MIB module are indexed by ifIndex.
dot11TxBFConfigTable
OID | Name | Type | Access
.1 | ReceiveStaggerSoundingOptionImplemented | ENUM | R
.2 | TransmitStaggerSoundingOptionImplemented | ENUM | R
.3 | ReceiveNDPOptionImplemented | ENUM | R
.4 | TransmitNDPOptionImplemented | ENUM | R
.5 | ImplicitTxBFOptionImplemented | ENUM | R
.6 | CalibrationOptionImplemented | ENUM | R
.7 | ExplicitCSITxBFOptionImplemented | ENUM | R
.8 | ExplicitNonCompressedbeamformingMatrixOptionImplemented | ENUM | R
.9 | ExplicitBFCSIFeedbackOptionImplemented | ENUM | R
.10 | ExplicitNonCompressedbeamformingMatrixFeedbackOptionImplemented | ENUM | R
.11 | ExplicitCompressedbeamformingMatrixFeedbackOptionImplemented | ENUM | R
.12 | NumberBeamFormingCSISupportAntenna | INTEGER | R
.13 | NumberNonCompressedbeamformingMatrixSupportAntenna | INTEGER | R
.14 | NumberCompressedbeamformingMatrixSupportAntenna | INTEGER | R
.15 | MaxCSIFeedbackDelay | Unsigned32 | R
ReceiveStaggerSoundingOptionImplemented
This attribute, when TRUE, indicates that the STA implementation supports the receiving of staggered sounding frames. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
TransmitStaggerSoundingOptionImplemented
This attribute, when TRUE, indicates that the STA implementation supports the transmission of staggered sounding frames. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
ReceiveNDPOptionImplemented
This attribute, when TRUE, indicates that the STA implementation is capable of receiving NDP as sounding frames. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
TransmitNDPOptionImplemented
This attribute, when TRUE, indicates that the STA implementation is capable of transmitting NDP as sounding frames. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
ImplicitTxBFOptionImplemented
This attribute, when TRUE, indicates that STA implementation is capable of applying implicit transmit beamforming. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
CalibrationOptionImplemented
This attribute indicates the level of calibration supported by the STA implementation. The default value of this attribute is 0. Enumerations: inCapable (0) unableToInitiate (1) ableToInitiate (2) fullyCapable (3)
ExplicitCSITxBFOptionImplemented
This attribute, when TRUE, indicates that STA implementation is capable of applying transmit beamforming using CSI explicit feedback in its transmission. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
ExplicitNonCompressedbeamformingMatrixOptionImplemented
This attribute, when TRUE, indicates that STA implementation is capable of applying transmit beamforming using non-compressed beamforming matrix explicit feedback in its transmission. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
ExplicitBFCSIFeedbackOptionImplemented
This attribute indicates the level of CSI explicit feedback returned by the STA implementation. The default value of this attribute is 0. Enumerations: inCapable (0) delayed (1) immediate (2) unsolicitedImmediate (3) aggregated (4) delayedAggregated (5) immediateAggregated (6) unsolicitedImmediateAggregated (7)
ExplicitNonCompressedbeamformingMatrixFeedbackOptionImplemented
This attribute indicates the level of non-compressed beamforming matrix explicit feedback returned by the STA implementation. The default value of this attribute is 0. Enumerations: inCapable (0) delayed (1) immediate (2) unsolicitedImmediate (3) aggregated (4) delayedAggregated (5) immediateAggregated (6) unsolicitedImmediateAggregated (7)
ExplicitCompressedbeamformingMatrixFeedbackOptionImplemented
This attribute indicates the level of non-compressed beamforming matrix explicit feedback returned by the STA implementation. The default value of this attribute is 0. Enumerations: inCapable (0) delayed (1) immediate (2) unsolicitedImmediate (3) aggregated (4) delayedAggregated (5) immediateAggregated (6) unsolicitedImmediateAggregated (7)
NumberBeamFormingCSISupportAntenna
This attribute indicates the maximum number of beamform antennas the beamformee can support when CSI feedback is required. Range: 1 to 4
NumberNonCompressedbeamformingMatrixSupportAntenna
This attribute indicates the maximum number of beamform antennas the beamformee can support when non-compressed beamforming matrix feedback is required. Range: 1 to 4
NumberCompressedbeamformingMatrixSupportAntenna
This attribute indicates the maximum number of beamform antennas the beamformee can support when compressed beamforming matrix feedback is required. Range: 1 to 4
MaxCSIFeedbackDelay
This attribute indicates the maximum allowed delay in microseconds between the transmission time of a sounding packet and the time a feedback response arrives (9.17.3 (Explicit feedback beamforming)) Range: 1 to -1

MIB Reference to Software Version 9.1.9 generated on 2014/07/17. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH