>> MIB - Management Information Base
>> Table: wlcWlanHWTable - (.1.3.6.1.4.1.272.4.61.1.24.1)
Description: This table lists all features of supported wireless cards.
wlcWlanHWTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | Name | DisplayString | R
.3 | TxPowerSteps | DisplayString | R
.4 | ShortRetries | ENUM | R
.5 | LongRetries | ENUM | R
.6 | FragmentationThreshold | ENUM | R
.7 | NoSpatialRx | INTEGER | R
.8 | NoSpatialTx | INTEGER | R
.9 | Bands | BITS | R
.10 | Modes | BITS | R
.11 | Bandwidth | ENUM | R
.12 | ShortGI | ENUM | R
.13 | Greenfield | ENUM | R
.14 | RxSTBC | ENUM | R
.15 | TxSTBC | ENUM | R
.16 | SkipModes | BITS | R
Index
Unique WLAN hardware index.
Name
Name of the WLAN hardware. Length: 0 to 32
TxPowerSteps
The steps of the TX power the wireless card supports. Length: 0 to 64
ShortRetries
This variable says if the wireless card supports the configuration of the short retry value or not. Default is false. Enumerations: true (1) false (2)
LongRetries
This variable says if the wireless card supports the configuration of the long retry value or not. Default is false. Enumerations: true (1) false (2)
FragmentationThreshold
This variable says if the wireless card supports the configuration of the fragmentation threshold value or not. Enumerations: true (1) false (2)
NoSpatialRx
This attribute indicates the number of receivable spatial streams. Range: 1 to 8
NoSpatialTx
This attribute indicates the maximum of transmittable spatial streams. Range: 1 to 8
Bands
The supported WLAN bands. Enumerations: band24 (0) band5 (1) band58 (2)
Modes
The Supported WLAN modes. Enumerations: m802-11a (0) m802-11b (1) m802-11g (2) m802-11n (3)
Bandwidth
The supported bandwidth capabilities of the radio. In case of false only 20MHz bandwidth is supported. In case of true also 40MHz bandwidth is supported. Enumerations: true (1) false (2)
ShortGI
This attribute, when TRUE, indicates that the Short Guard option is implemented. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
Greenfield
This attribute, when TRUE, indicates that the HT Greenfield option is implemented. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
RxSTBC
This attribute, when TRUE, indicates that the entity is capable of receiving frames that are sent using the Space-Time Block Code (STBC). The default value of this attribute is FALSE. Enumerations: true (1) false (2)
TxSTBC
This attribute, when TRUE, indicates that the entity is capable of transmitting frames using Space-Time Block Code (STBC) option. The default value of this attribute is FALSE. Enumerations: true (1) false (2)
SkipModes
This variable says which modes of the WlanIfSkipChannels the wireless card supports. Enumerations: ap24ghz (0) ap5ghz (1) client24ghz (2) client5ghz (3)

MIB Reference to Software Version 9.1.9 generated on 2014/07/17. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH