>> MIB - Management Information Base
>> Table: userAlertTable - (.1.3.6.1.4.1.272.4.62.1.1.1)
Description: Contents the notification Entry.
userAlertTable
OID | Name | Type | Access
.1 | Address | DisplayString | RW
.2 | Rule | DisplayString | RW
.3 | Timeout | INTEGER | RW
.4 | Count | INTEGER | RW
.5 | Compress | ENUM | D
.6 | Level | ENUM | RW
.7 | Mask | INTEGER | RW
.8 | Subject | DisplayString | RW
.9 | Bits | BITS | RW
.10 | Service | ENUM | RW
Address
The E-Mail recipient of a notification or the subscriber number of a SMS capable (mobile) device.
Rule
The expression which is searched for in the syslog message.
Timeout
The time after which the E-Mail or SMS is forced to be sent.
Count
The count of messages to be collected after which the E-Mail is forced to be sent. Since SMS is restricted to 160 characters this object is ignored for SMS.
Compress
Definition for userAlertService E-Mail: Declares whether identical messages should just be displayed once followed by the message: `This Message was repeated xxTimes'. Definition for userAlertService SMS: When enabled the syslog message timestamp is suppressed to save space for the message text.
Level
The syslog level of the syslog message to be searched for.
Mask
The Subtypes of Message watching.
Subject
Defines the subject of the email message.
Bits
The subjects of the syslog message for which user alert shall be active.
Service
The service which is used to deliver the alert.

MIB Reference to Software Version 9.1.9 generated on 2014/07/17. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH