>> MIB - Management Information Base
>> Table: ipMRoute - (.1.3.6.1.2.1.83.1.1)
ipMRoute
OID | Name | Type | Access
.1 | Enable | ENUM | RW
.7 | EntryCount | Gauge32 | R
Enable
The enabled status of IP Multicast routing on this router. Enumerations: enabled (1) disabled (2)
EntryCount
The number of rows in the ipMRouteTable. This can be used to monitor the multicast routing table size.

MIB Reference to Software Version 9.1.9 generated on 2014/07/17. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH