>> MIB - Management Information Base
>> Table: ospfVirtNbrTable - (.1.3.6.1.2.1.14.11.1)
Description: Virtual neighbor information.
ospfVirtNbrTable
OID | Name | Type | Access
.1 | Area | IpAddress | R
.2 | RtrId | IpAddress | R
.3 | IpAddr | IpAddress | R
.4 | Options | INTEGER | R
.5 | State | ENUM | R
.6 | Events | Counter | R
.7 | LsRetransQLen | Gauge | R
.8 | HelloSuppressed | ENUM | R
Area
The Transit Area Identifier.
RtrId
A 32-bit integer uniquely identifying the neighboring router in the Autonomous System.
IpAddr
The IP address this Virtual Neighbor is us- ing.
Options
A Bit Mask corresponding to the neighbor's op- tions field. Bit 1, if set, indicates that the system will operate on Type of Service metrics other than TOS 0. If zero, the neighbor will ignore all metrics except the TOS 0 metric. Bit 2, if set, indicates that the system is Network Multicast capable; ie, that it imple- ments OSPF Multicast Routing.
State
The state of the Virtual Neighbor Relation- ship. Enumerations: down (1) attempt (2) init (3) twoWay (4) exchangeStart (5) exchange (6) loading (7) full (8)
Events
The number of times this virtual link has changed its state, or an error has occurred.
LsRetransQLen
The current length of the retransmission queue.
HelloSuppressed
Indicates whether Hellos are being suppressed to the neighbor Enumerations: true (1) false (2)

MIB Reference to Software Version 9.1.9 generated on 2014/07/17. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH