>> MIB - Management Information Base
>> Table: ipDhcpClientRtTemplTable - (.1.3.6.1.4.1.272.4.5.52.9.1)
Description: Remark: Formally defined INDEX does not cover all entries that are needed for selecting an entry unambiguously. However, listing all of them would make the OIDs rather long.
ipDhcpClientRtTemplTable
OID | Name | Type | Access
.1 | RtType | ENUM | D
.2 | Description | DisplayString | RW
.3 | Metric1 | INTEGER | RW
.4 | DstIfIndex | INTEGER | RW
.5 | DstIfMode | ENUM | RW
.6 | DstAddr | IpAddress | RW
.7 | DstMask | IpAddress | RW
.8 | DstPort | INTEGER | RW
.9 | DstPortRange | INTEGER | RW
.10 | SrcIfIndex | INTEGER | RW
.11 | SrcAddr | IpAddress | RW
.12 | SrcMask | IpAddress | RW
.13 | SrcPort | INTEGER | RW
.14 | SrcPortRange | INTEGER | RW
.15 | Protocol | ENUM | RW
.16 | Tos | INTEGER | RW
.17 | TosMask | INTEGER | RW
RtType
Tells what kind of routing-entry shall be built. <ipextrt>: Build ipExtRtType-entry. <ipextrt>: Build ipRouteType-entry. <delete>: Remove this template-entry. Enumerations: ipextrt (1) iproute (2) delete (3)
Description
Copied to ipExtRtDescription if RtType is ipextrt. Ignored if RtType is iproute. Length: 0 to 255
Metric1
Copied to ipExtRtMetric1 if RtType is ipextrt. Copied to ipRouteMetric1 if RtType is iproute. Remark: Default-value deviates from ipExtRt/ipRoute-table
DstIfIndex
DHCP-client checks this value against its own interface to decide whether it shall use this pattern-entry. Copied to ipExtRtDstIfIndex if RtType is ipextrt. Copied to ipRouteIfIndex if RtType is iproute.
DstIfMode
Copied to ipExtRtDstIfMode if RtType is ipextrt. Ignored if RtType is iproute. Remark: Default-value deviates from ipExtRt-table Enumerations: dialup-wait (1) dialup-continue (2) up-only (3) always (4) dialup-always (5)
DstAddr
Copied to ipExtRtDstAddr if RtType is ipextrt. Copied to ipRouteDest if RtType is iproute.
DstMask
Copied to ipExtRtDstMask if RtType is ipextrt. Copied to ipRouteMask if RtType is iproute.
DstPort
Copied to ipExtRtDstPort if RtType is ipextrt. Ignored if RtType is iproute. Range: -1 to 65535
DstPortRange
Copied to ipExtRtDstPortRange if RtType is ipextrt. Ignored if RtType is iproute. Range: -1 to 65535
SrcIfIndex
Copied to ipExtRtSrcIfIndex if RtType is ipextrt. Ignored if RtType is iproute.
SrcAddr
Copied to ipExtRtSrcAddr if RtType is ipextrt. Ignored if RtType is iproute.
SrcMask
Copied to ipExtRtSrcMask if RtType is ipextrt. Ignored if RtType is iproute.
SrcPort
Copied to ipExtRtSrcPort if RtType is ipextrt. Ignored if RtType is iproute. Range: -1 to 65535
SrcPortRange
Copied to ipExtRtSrcPortRange if RtType is ipextrt. Ignored if RtType is iproute. Range: -1 to 65535
Protocol
Copied to ipExtRtProtocol if RtType is ipextrt. Ignored if RtType is iproute. Enumerations: icmp (1) igmp (2) ggp (3) tcp (6) egp (8) pup (12) udp (17) hmp (20) xns-idp (22) rdp (27) ipv6 (41) rsvp (46) gre (47) esp (50) ah (51) igrp (88) ospf (89) pim (103) l2tp (115) dont-verify (256)
Tos
Copied to ipExtRtTos if RtType is ipextrt. Ignored if RtType is iproute. Range: 0 to 255
TosMask
Copied to ipExtRtTosMask if RtType is ipextrt. Ignored if RtType is iproute. Range: 0 to 255

MIB Reference to Software Version 9.1.9 generated on 2014/07/17. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH