>> MIB - Management Information Base
>> Table: ipSifAliasServiceTable - (.1.3.6.1.4.1.272.4.5.29.1)
Description: Contains a alias Service Entry Protocol,Port,Range
ipSifAliasServiceTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | Alias | DisplayString | RW
.3 | Protocol | ENUM | D
.4 | Port | INTEGER | RW
.5 | Range | INTEGER | RW
.6 | Type | ENUM | R
.7 | Group | INTEGER | RW
.8 | SourcePort | INTEGER | RW
.9 | SourceRange | INTEGER | RW
.10 | IcmpType | INTEGER | RW
.11 | IcmpCode | INTEGER | RW
Index
The Index for the address alias
Alias
Alias Name for the Service Entry Length: 0 to 255
Protocol
The protocol for the Service alias Enumerations: icmp (1) igmp (2) ggp (3) ip (4) tcp (6) egp (8) igp (9) pup (12) chaos (16) udp (17) hmp (20) xns-idp (22) rdp (27) ipv6 (41) rsvp (46) gre (47) esp (50) ah (51) tlsp (56) skip (57) kryptolan (65) iso-ip (80) igrp (88) ospf (89) ipip (94) pim (103) ipx-in-ip (111) vrrp (112) l2tp (115) local (250) internet (251) netmeeting (252) udptcp (253) any (254) delete (255) dont-verify (256)
Port
The Port for the Service Alias. Range: -1 to 65535
Range
The Port Range for the Service Alias. Range: 1 to 65536
Type
Specifies wether created by the IP/SIF subsystem itself or created/modified by the administrator. Enumerations: predefined (1) custom (2)
Group
For values greater than zero this entry determines the IP service group this entry belongs to, see also ipSifAliasServiceGroupId
SourcePort
The Source Port for the Service Alias. Range: 0 to 65535
SourceRange
The Source Port Range for the Service Alias. Range: 1 to 65536
IcmpType
The ICMP Type for the Service Alias. Range: -1 to 255
IcmpCode
The ICMP Code for the Service Alias. Range: -1 to 255

MIB Reference to Software Version 9.1.9 generated on 2014/07/17. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH