>> MIB - Management Information Base
>> Table: msdpMeshGroupTable - (.1.3.6.1.4.1.272.4.5.56.1.1.7.1)
Description: An entry (conceptual row) representing a peer in an MSDP Mesh Group. If row creation is supported, dynamically added rows are added to the system's stable configuration (corresponding to a StorageType value of nonVolatile).
msdpMeshGroupTable
OID | Name | Type | Access
.1 | Name | DisplayString | RC
.2 | PeerAddress | IpAddress | RC
.3 | Status | ENUM | D
Name
The name of the mesh group. Length: 1 to 64
PeerAddress
A peer address that is a member of the mesh group with name msdpMeshGroupName. The msdpMeshGroupPeerAddress must match a row in the msdpPeerTable.
Status
This entry's status, by which new entries may be added to the table and old entries deleted. msdpMeshGroupName and msdpMeshGroupPeerAddress must be set to valid values before the row can be activated. Since these are the table's INDEX, a row can be activated by simply setting the msdpMeshGroupStatus variable. It is not possible to modify other columns in the same conceptual row when the status value is active(1), because the only other objects in the row are part of the INDEX. Changing one of these changes the row, so an old row must be deleted and a new one created. Enumerations: active (1) notInService (2) notReady (3) createAndGo (4) createAndWait (5) destroy (6)

MIB Reference to Software Version 9.1.9 generated on 2014/07/17. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH