>> MIB - Management Information Base
>> Table: frErrTable - (.1.3.6.1.2.1.10.32.3.1)
Description: The error information for a single frame relay interface.
frErrTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | R
.2 | Type | ENUM | R
.3 | Data | OCTET STRING | R
.4 | Time | TimeTicks | R
IfIndex
The ifIndex Value of the corresponding ifEn- try.
Type
The type of error that was last seen on this interface. Enumerations: unknownError (1) receiveShort (2) receiveLong (3) illegalDLCI (4) unknownDLCI (5) dlcmiProtoErr (6) dlcmiUnknownIE (7) dlcmiSequenceErr (8) dlcmiUnknownRpt (9) noErrorSinceReset (10)
Data
An octet string containing as much of the er- ror packet as possible. As a minimum, it must contain the Q.922 Address or as much as was delivered. It is desirable to include all in- formation up to the PDU.
Time
The value of sysUpTime at which the error was detected.

MIB Reference to Software Version 9.1.9 generated on 2014/07/17. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH