>> MIB - Management Information Base
>> Table: vmsMessageTable - (.1.3.6.1.4.1.272.4.34.1.5.1)
Description: This table lists the received messages.
vmsMessageTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | AccountIdx | AccountIndex | R
.3 | Caller | DisplayString | R
.4 | Received | Date | R
.5 | File | DisplayString | R
.6 | Status | ENUM | R
.7 | AdminStatus | ENUM | D
.8 | AccessStatus | BITS | R
Index
Unique Index of the received message.
AccountIdx
Number of the associated Voice extension (reference to the vmsAccountTable). Range: 1 to 65535
Caller
Originator of the message. Length: 0 to 255
Received
Time and Date of the message. Range: 0 to -1
File
Message file name. Length: 0 to 255
Status
Status of the messages. new(1) : new unheard message old(2) : heard message saved(3): message was heared and saved Enumerations: new (1) old (2) saved (3)
AdminStatus
Admin status of the messages. enabled(1): no action for this message active move-to-old(2): new message should be moved to old move-to-saved(3): now/old message should be moved to saved delete(4) : message should be deleted Enumerations: enabled (1) move-to-old (2) move-to-saved (3) delete (4)
AccessStatus
Access flags. playing : read access for playing sending : read access for sending e-mail recording: write access for recording Enumerations: playing (0) sending (1) recording (2)

MIB Reference to Software Version 9.1.9 generated on 2014/07/17. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH