>> MIB - Management Information Base
>> Table: sysPCMTable - (.1.3.6.1.4.1.272.4.17.1.1)
sysPCMTable
OID | Name | Type | Access
.1 | Slot | INTEGER | R
.2 | Unit | INTEGER | R
.3 | ClockStatus | ENUM | R
.4 | ClockMaster | ENUM | R
.5 | MasterPrio | INTEGER | RW
.10 | Changes | Counter | R
Slot
description not available Range: 0 to 30
Unit
Identification number of the used unit. Range: -1 to 31
ClockStatus
shows wether this board can supply a clock signal to the internal PCM-Highway. ready: this board can supply a clock signal not_ready: this board can't supply a clock signal Enumerations: ready (1) not-ready (2)
ClockMaster
shows the status of this board. candidate: this board can become PCM Highway master master: this board is PCM Highway master Enumerations: candidate (1) master (2)
MasterPrio
Priority during PCM-Highway master election. A small value results in high priority; the candidate with highest priority wins the election. Prio 128 (lowest priority) lets the PCM-Highway master use its own clock (instead of using network clock). Range: 0 to 128
Changes
counts how often sysPCMClockMaster has changed.

MIB Reference to Software Version 9.1.9 generated on 2014/07/17. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH