>> MIB - Management Information Base
>> Table: sysConfigAdmin - (.1.3.6.1.4.1.272.4.17.9.1)
sysConfigAdmin
OID | Name | Type | Access
.1 | LedMode | ENUM | RW
.2 | TftpBootLocalIpAddr | IpAddress | RW
.3 | TftpBootServerIpAddr | IpAddress | RW
.4 | TftpBootFile | DisplayString | RW
.5 | AutoTftpBoot | ENUM | RW
LedMode
The LED mode of the system: normal : LEDs work normal, minimal : only Status-LED flashes once in a second, off := LEDs are off. Enumerations: normal (1) minimal (2) off (3)
TftpBootLocalIpAddr
Local IP address for TFTP boot.
TftpBootServerIpAddr
IP address of TFTP sever.
TftpBootFile
Name of the TFTP boot file. Length: 0 to 255
AutoTftpBoot
Indicates whether the device tries to boot the image from TFTP server. If this fails it will stay in the bootmonitor mode. Enumerations: no (1) yes (2)

MIB Reference to Software Version 9.1.9 generated on 2014/07/17. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH