>> MIB - Management Information Base
>> Table: mpsArsRoutingDetailsTable - (.1.3.6.1.4.1.272.4.53.10.5.1)
Description: This table assigns a carrier and start time selection to an entry in the mpsArsRoutingTable.
mpsArsRoutingDetailsTable
OID | Name | Type | Access
.1 | Hour | INTEGER | RW
.2 | Minute | INTEGER | RW
.3 | RoutingIndex | RouteIndex | RW
.4 | CarrierIndex | CarrierIndex | RW
.5 | AdminStatus | ENUM | D
Hour
This object specifies the start hour for activity of this routing entry. Range: 0 to 23
Minute
This object specifies the start minute for activity of this routing entry. Range: 0 to 59
RoutingIndex
This object specifies a number for the LCR zone. Reference to mpsARSZoneIndex.
CarrierIndex
A unique index for each carrier. Reference to mpsARSCarrierIndex.
AdminStatus
Specifies whether this entry defines a LCR RoutingDetails Entry or should be deleted Enumerations: enable (1) delete (2)

MIB Reference to Software Version 9.1.9 generated on 2014/07/17. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH