>> MIB - Management Information Base
>> Table: ipDhcpPoolTable - (.1.3.6.1.4.1.272.4.5.52.3.1)
Description: This table defines for DHCP which dynamic IP address pool, represented by an entry in ipDynAddrPoolTable, is to be used on which interface.
ipDhcpPoolTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | RW
.2 | DynAddrPoolId | DynIpPoolId | RW
.3 | AssignmentMode | BITS | RW
.4 | Enabled | ENUM | D
.5 | LeaseTime | INTEGER | RW
.6 | Gateway | IpAddress | RW
.7 | RadiusAcct | ENUM | RW
.8 | RadiusGroupId | INTEGER | RW
.9 | AliveCheck | ENUM | RW
.10 | AliveInterval | INTEGER | RW
.11 | TftpServer1 | IpAddress | RW
.12 | TftpServer2 | IpAddress | RW
.13 | OfferOptionsGroupID | INTEGER | RW
.14 | AckOptionsGroupID | INTEGER | RW
.15 | GatewayEnabled | ENUM | RW
.16 | SendRepliesToRelay | ENUM | RW
IfIndex
The index for the interface for which the DHCP subsystem is answering DHCP requests using the associated dynamic address pool.
DynAddrPoolId
Uniquely identifies associated dynamic address pool from which the DHCP requests are served from. Range: 0 to 65535
AssignmentMode
Indicates, to which DHCP clients addresses from the associated dynamic address pool will be assigned: to clients in local network (local) or/and to clients that ask for ip address via a BOOTP relay agent (relay). Enumerations: local (0) relay (1)
Enabled
Enable, disable or delete the table entry. Enumerations: false (1) true (2) delete (3)
LeaseTime
Specifies the amount of time (in minutes) IP addresses of the associated pool are leased to clients. If in case of manual assigned IP address ipStatAddrLeaseTime value is specified (i.e. is not -1), ipDhcpPoolLeaseTime is ignored in favor of this parameter. Range: 1 to 300
Gateway
The default gateway given to the client via 'router option'. An IP address of 0.0.0.0 uses the local IP address of the interface where the request came in if the server and client are located in the same network. If the server and the client not located in the same network, the address of the BOOTP relay agent forwarding the request is used. If in case of manual assigned IP address ipStatAddrGateway value is specified (i.e. is not 255.255.255.255), ipDhcpPoolGateway is ignored in favor of this parameter.
RadiusAcct
Enables or disables the radius accounting for IP addresses of the associated pool: - disabled : disables radius accounting - enabled : enables radius accounting If in case of manual assigned IP address ipStatAddrRadiusAcct value is specified (i.e. is not default), ipDhcpPoolRadiusAcct is ignored in favor of this parameter. Enumerations: disabled (2) enabled (3)
RadiusGroupId
This object specifies the radius group Id which is used by the radius daemon to find the associated server entry in radiusSrvTable for accounting purposes. See description of radiusSrvGroupId for details. If in case of manual assigned IP address ipStatAddrRadiusGroupId value is specified (i.e. is not -1), ipDhcpPoolRadiusGroupId is ignored in favor of this parameter.
AliveCheck
Enables or disables the alive checking for the associated pool. The alive check allows the system to purge dynamic entries whose lease is still valid but the client no longer exists. - disabled : disables alive check for pool users - enabled : enables alive check for pool users Enumerations: disabled (1) enabled (2)
AliveInterval
This object specifies a time period in seconds for checking whether the client is still alive. If this object is set to 0, no alive check is performed. If in case of manual assigned IP address ipStatAddrAliveInterval value is specified (i.e. is not -1), ipDhcpPoolAliveInterval is ignored in favor of this parameter.
TftpServer1
The IP address of the first TFTP server given to the client via 'TFTP server option' (DHCP option 150). If in case of manual assigned IP address either ipStatAddrTftpServer1 or ipStatAddrTftpServer2 value is assigned (i.e. is not 255.255.255.255), ipDhcpPoolTftpServer1 and ipDhcpPoolTftpServer2 are ignored in favor of these parameters. If ipDhcpPoolTftpServer1 is 0.0.0.0, then only the IP address specified in ipDhcpPoolTftpServer2 will be considered. If both addresses are 0.0.0.0, no DHCP option 150 will be returned to the client.
TftpServer2
The IP address of the second TFTP server given to the client via 'TFTP server option' (DHCP option 150). If in case of manual assigned IP address either ipStatAddrTftpServer1 or ipStatAddrTftpServer2 value is assigned (i.e. is not 255.255.255.255), ipDhcpPoolTftpServer1 and ipDhcpPoolTftpServer2 are ignored in favor of these parameters. If ipDhcpPoolTftpServer2 is 0.0.0.0, then only the IP address specified in ipDhcpPoolTftpServer1 will be considered. If both addresses are 0.0.0.0, no DHCP option 150 will be returned to the client.
OfferOptionsGroupID
Identifies the option or set of options which are added to the original DHCP OFFER message issued by the DHCP server before delivering it to the DHCP client. The options are defined in ipDhcpOptionTable. Selecting a null value result in no option being added. In case of manual assigned IP address ipStatAddrOfferOptionsGroupId defines the used group id and ipDhcpPoolOfferOptionsGroupID is ignored. Range: 0 to 65535
AckOptionsGroupID
Identifies the option or set of options which are added to the original DHCP ACK message issued by the DHCP server before delivering it to the DHCP client. The options are defined in ipDhcpOptionTable. Selecting a null value result in no option being added. In case of manual assigned IP address ipStatAddrAckOptionsGroupId defines the used group id and ipDhcpPoolAckOptionsGroupID is ignored. Range: 0 to 65535
GatewayEnabled
Specifies if 'router option' is delivered within BOOTP REPLY message. If this object is set to 'yes' router option is filled depending on ipDhcpPoolGateway. If this object is set to 'no' router option is not delivered regardless of object ipDhcpPoolGateway. In case of manual assigned IP address ipStatAddrGatewayEnabled defines wether 'router option' is delivered or not and ipDhcpPoolGatewayEnabled is ignored. Enumerations: yes (1) no (2)
SendRepliesToRelay
As soon as a DHCP request includes a client IP address (ciaddr), RFC 1542 recommends that the server unicast the relevant DHCP reply message to the client IP address. Nevertheless, situations exist where it is desirable to send the reply to a BOOTP relay IP address if one has been included in the DHCP request. This object specifies how the DHCP server must behave in this aspect: - If this object is set to 'no' (default) and a client IP address was included in the DHCP request, DHCP replies are sent to this client IP address, regardless of a BOOTP relay address being included or not in the DHCP request. - If this object is set to 'yes' and a BOOTP relay IP address was included in the DHCP request, DHCP replies are sent to this BOOTP relay IP address, regardless of a client IP address being included or not in the DHCP request. Enumerations: yes (1) no (2)

MIB Reference to Software Version 9.1.9 generated on 2014/07/17. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH