>> MIB - Management Information Base
>> Table: greIfTable - (.1.3.6.1.4.1.272.4.23.5.1)
Description: Entries in this table are created by defining a new value for the field greDstIpAddr. Entries may be deleted by setting the field greUseKey to 'delete'.
greIfTable
OID | Name | Type | Access
.1 | IfIndex | INTEGER | R
.2 | IfDescr | DisplayString | RW
.3 | IfMtu | INTEGER | RW
.4 | DstIpAddr | IpAddress | RW
.5 | Key | INTEGER | RW
.6 | UseKey | ENUM | D
.7 | SrcIpAddr | IpAddress | RW
IfIndex
The index of the virtual interface. This object identifies a row in the ifTable.
IfDescr
The name of the virtual interface. The same name will be assigned to the corresponding ifDescr in the ifTable. Length: 0 to 255
IfMtu
Determines size of the largest datagram which can be sent on the interface, specified in octets (see ifMtu). Range: 1 to 8192
DstIpAddr
The IP address of the GRE remote partner.
Key
The optional 32-bit key for this GRE tunnel. Multiple tunnels can be used simultaneously between the two same GRE partners provided each tunnel uses a different key.
UseKey
This object indicates, whether the key value specified in greKey should be processed in GRE headers. Enumerations: delete (1) yes (2) no (3)
SrcIpAddr
The source IP address used when sending GRE packets. If this value is set to 0.0.0.0, the IP address of the interface used to route packets towards the remote partner will be automatically selected for this purpose.

MIB Reference to Software Version 9.1.9 generated on 2014/07/17. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH