>> MIB - Management Information Base
>> Table: pimSGRptTable - (.1.3.6.1.4.1.272.4.5.54.2.1.8.1)
Description: An entry (conceptual row) in the pimSGRptTable.
pimSGRptTable
OID | Name | Type | Access
.1 | SrcAddress | InetAddressIPv6 | R
.2 | UpTime | TimeTicks | R
.3 | UpstreamPruneState | ENUM | R
.4 | UpstreamOverrideTimer | TimeTicks | R
.5 | RPFNextHopType | ENUM | R
.6 | RPFNextHop | InetAddressIPv6 | R
SrcAddress
The source address for this entry. The InetAddressType is given by the pimStarGAddressType object. Length: 16 to 16
UpTime
The time since this entry was created by the local router.
UpstreamPruneState
Whether the local router should prune the source off the RP tree. This corresponds to the state of the upstream (S,G,rpt) state machine for triggered messages in the PIM-SM specification. Enumerations: rptNotJoined (1) pruned (2) notPruned (3)
UpstreamOverrideTimer
The time remaining before the local router sends a triggered (S,G,rpt) Join message on pimStarGRPFIfIndex. This timer is called the (S,G,rpt) Upstream Override Timer in the PIM-SM specification. This object is zero if the timer is not running.
RPFNextHopType
The address type of the RPF next hop towards the RP, or unknown(0) if the RPF next hop is unknown. Enumerations: unknown (0) ipv4 (1) ipv6 (2) ipv4z (3) ipv6z (4) dns (16)
RPFNextHop
The address of the RPF next hop towards the RP. The InetAddressType is given by the pimStarGRPFNextHopType object. Length: 16 to 16

MIB Reference to Software Version 9.1.9 generated on 2014/07/17. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH