>> MIB - Management Information Base
>> Table: pimStarStarRPTable - (.1.3.6.1.4.1.272.4.5.54.2.1.103.1)
Description: An entry (conceptual row) in the pimStarStarRPTable.
pimStarStarRPTable
OID | Name | Type | Access
.1 | AddressType | ENUM | R
.2 | Address | InetAddressIPv6 | R
.3 | UpTime | TimeTicks | R
.4 | UpstreamJoinTimer | TimeTicks | R
.5 | UpstreamJoinState | ENUM | R
.6 | UpstreamNeighborType | ENUM | R
.7 | UpstreamNeighbor | InetAddressIPv6 | R
.8 | Local | ENUM | R
AddressType
The address type of this RP. Enumerations: unknown (0) ipv4 (1) ipv6 (2) ipv4z (3) ipv6z (4) dns (16)
Address
The address of this RP. Length: 16 to 16
UpTime
The time since this RP exists.
UpstreamJoinTimer
The Upstream Join/Prune Timer is used to send out periodic Join(*,*,RP) messages, and to override Prune(*,*,RP) messages from peers on an upstream LAN interface.
UpstreamJoinState
The upstream (*,*,RP) Join/Prune State reflects the state of the upstream (*,*,RP) state machine in the PIM-SM specification. Enumerations: notJoined (1) joined (2)
UpstreamNeighborType
The primary address type of the upstream neighbor, or unknown(0) if the upstream neighbor address is unknown or is not a PIM neighbor. Enumerations: unknown (0) ipv4 (1) ipv6 (2) ipv4z (3) ipv6z (4) dns (16)
UpstreamNeighbor
The primary address of the neighbor on pimStarStarRPIfIndex. The InetAddressType is given by the pimStarStarRPUpstreamNeighborType object. Length: 16 to 16
Local
Whether this RP is the local router. Enumerations: true (1) false (2)

MIB Reference to Software Version 9.1.9 generated on 2014/07/17. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH