>> MIB - Management Information Base
>> Table: ipSifExpectTable - (.1.3.6.1.4.1.272.4.5.35.1)
Description: Contains expected Sessions with Source Destination
ipSifExpectTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | Source | IpAddress | R
.3 | Destination | IpAddress | R
.4 | Protocol | ENUM | D
.5 | SourcePort | INTEGER | R
.6 | DestPort | INTEGER | R
.7 | Priority | ENUM | R
.8 | ClassId | INTEGER | R
.9 | IfIndex | INTEGER | R
Index
This field is used for SIF-internal signalling and stores the index for the expected session for later matching.
Source
The source-IP-address for the expected session. A value of 0 means ANY source-address.
Destination
The destination-IP-address for the expected session. A value of 0 means ANY destination-address.
Protocol
The protocol of the expected session. Enumerations: igmp (2) ip (4) tcp (6) udp (17) delete (255)
SourcePort
The source-port-number of the expected session. A value of 0 means ANY source-port-number.
DestPort
The destination-port-number of the expected session. A value of 0 means ANY destination-port-number.
Priority
Defines the QoS-priority/policy to be used for the expected SIF-session. Enumerations: default (1) low-latency (2) high (3) medium (4) low (5)
ClassId
Internal ID for mapping SIF-policy to QoS-policy. Default-value of 0 means NOT SPECIFIED. Range: 1 to 255
IfIndex
Interface-index for which the session is expected. A value of 0 means ANY interface-index.

MIB Reference to Software Version 9.1.9 generated on 2014/07/17. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH