>> MIB - Management Information Base
>> Table: ipsecLifeTimeTable - (.1.3.6.1.4.1.272.4.26.9.1)
Description: This object contains a lifetime, i.e. the soft and hard expiry limits for IPsec and IKE SA's. The usage of this table is deprecated, use the ikePrfLifeXxx and ipsecPrfLifeXxx variables in the ikeProfileTable and ipsecProfileTable directly instead.
ipsecLifeTimeTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.2 | Type | ENUM | D
.5 | HardKb | INTEGER | R
.6 | HardSec | INTEGER | R
.7 | Policy | ENUM | R
.8 | SoftPercent | INTEGER | R
Index
A unique index identifying this entry.
Type
This object specifies the type of a lifetime entry. Enumerations: delete (1) generic (2)
HardKb
The maximum amount of data (in KB) which may be protected by an SA before it is deleted.
HardSec
The maximum time (in seconds) after which an SA will be refreshed,.
Policy
This object specifies the way the lifetime information is applied. Possible values: loose(1), -- accept and use anything proposed strict(2), -- accept and use only what is configured notify(3) -- accept anything, if own values are smaller than what was proposed use these and send responder lifetime notification. Enumerations: loose (1) strict (2) notify (3)
SoftPercent
The percentage of the hard lifetimes (traffic and time based) after which rekeying is started. Range: 50 to 100

MIB Reference to Software Version 9.1.9 generated on 2014/07/17. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH