>> MIB - Management Information Base
>> Table: ikeSaTable - (.1.3.6.1.4.1.272.4.26.4.1)
Description: This object contains an IKE security association.
ikeSaTable
OID | Name | Type | Access
.1 | Index | INTEGER | R
.3 | State | ENUM | D
.4 | XchType | ENUM | R
.5 | AuthMethod | ENUM | R
.7 | Role | ENUM | R
.8 | LocalId | DisplayString | R
.9 | RemoteId | DisplayString | R
.10 | LocalIp | IpAddress | R
.11 | RemoteIp | IpAddress | R
.12 | CookieI | OCTET STRING | R
.13 | CookieR | OCTET STRING | R
.15 | NumCerts | INTEGER | R
.16 | NumNegotiations | INTEGER | R
.17 | Bytes | INTEGER | R
.18 | MajVersion | INTEGER | R
.19 | MinVersion | INTEGER | R
.20 | PeerIndex | INTEGER | R
.21 | HeartbeatsEnabled | ENUM | R
.22 | HeartbeatsSent | INTEGER | R
.23 | HeartbeatsReceived | INTEGER | R
.24 | Created | Date | R
.25 | LastUsed | Date | R
.26 | EncAlg | ENUM | R
.27 | HashAlg | ENUM | R
.28 | PrfAlg | ENUM | R
.29 | Expires | Date | R
.30 | LocalPort | INTEGER | R
.31 | RemotePort | INTEGER | R
.32 | XauthType | ENUM | R
.33 | XauthUser | DisplayString | R
.34 | Ip6LocalIp | InetAddressIPv6 | R
.35 | Ip6RemoteIp | InetAddressIPv6 | R
Index
A unique index for this entry.
State
This object specifies the state of the SA. Possible values: negotiating(1), -- the SA is still being negotiated established(2), -- the SA negotiation is finished waiting-for-remove(3), -- the SA is waiting for removal delete(7) -- mark the SA for deletion. Enumerations: negotiating (1) established (2) waiting-for-remove (3) delete (7)
XchType
The exchange mode used to create the SA. Possible values: base(1), -- IKE base mode mode id-protect(2), -- IKE identity protection -- (oakley main mode) authentication-only(3), -- Authentication only mode aggressive(4), -- IKE (oakley) aggressive mode info(5), -- IKE informational exchange mode quick(32), -- IKE quick mode new-group(33), -- IKE new group mode any(256) -- Other mode. Enumerations: base (1) id-protect (2) aggressive (4) any (256)
AuthMethod
The authenticatin method used when negotiating this SA. Possible values: pre-sh-key(1), -- Authentication using pre shared keys dss-sig(2), -- Authentication using DSS signatures rsa-sig(3), -- Authentication using RSA signatures rsa-enc(4), -- Authentication using RSA encryption rsa-enc-rev(5) -- Authentication using revised RSA encryption. Enumerations: pre-sh-key (1) dss-sig (2) rsa-sig (3) rsa-enc (4) rsa-enc-rev (5)
Role
This object specifies by which side the SA negotiation was initiated. Possible values: initiator(1), -- this end initiated the SA negotiation responder(2) -- the remote end initiated the SA negotiation. Enumerations: initiator (1) responder (2)
LocalId
The local ID used for authentication. Length: 0 to 255
RemoteId
The remote ID used for authentication. Length: 0 to 255
LocalIp
The local IP address used in the IKE communication.
RemoteIp
The remote IP address used in the IKE communication.
CookieI
The cookie of the initiator.
CookieR
The cookie of the responder.
NumCerts
The number of certificates received from the remote side when negotiating this SA.
NumNegotiations
This object specifies the number of currently active negotiations for this SA.
Bytes
Number of bytes transmitted using this SA.
MajVersion
The IKE major version number.
MinVersion
The IKE minor version number.
PeerIndex
The index of the peer for which this SA was created.
HeartbeatsEnabled
This object specifies whether heartbeats are sent/expected over this SA possible values: send(1), -- send heartbeats expect(2), -- expect heartbeats both(3), -- send and expect heartbeats none(4) -- neither send nor expect heartbeats. Enumerations: send (1) expect (2) both (3) none (4)
HeartbeatsSent
Number of Heartbeats sent over this SA.
HeartbeatsReceived
Number of Heartbeats received over this SA.
Created
Time the SA was created. Range: 0 to -1
LastUsed
Time the SA was used last. Range: 0 to -1
EncAlg
The encryption algorithm used. Enumerations: des (1) idea (2) blowfish (3) rc5 (4) des3 (5) cast128 (6) aes (7) twofish (9)
HashAlg
The hash algorithm used. Enumerations: md5 (1) sha (2) tiger (3) ripemd160 (4)
PrfAlg
The hash algorithm used for the pseudo random function. Enumerations: md5 (1) sha (2) tiger (3) ripemd160 (4)
Expires
Time the SA will expire. Range: 0 to -1
LocalPort
Local port currently used for the SA. Range: 0 to 65535
RemotePort
Remote port currently used for the SA. Range: 0 to 65535
XauthType
This object displayes whether XAUTH is used or not after complete establishment of the SA. If XAUTH is used then the type of the extended authentication is displayed. Enumerations: generic (0) radius-chap (1) otp (2) s-key (3) none (32768)
XauthUser
User name used for Extended Authentication. Length: 0 to 255
Ip6LocalIp
The local IPv6 address used in the IKE communication.
Ip6RemoteIp
The remote IPv6 address used in the IKE communication.

MIB Reference to Software Version 9.1.9 generated on 2014/07/17. Provided by webmaster@bintec-elmeg.com Copyright ©2014 by bintec elmeg GmbH